1、功能说明
    1、通过设定闹钟时间来触发闹钟中断。
    2、通过闹钟标志位来配置IO输出

2、使用环境

    软件开发环境：KEIL MDK-ARM V5.25
    硬件环境：
        1、基于评估板N32G4FRML-STB V1.1开发
        2、MCU：N32G4FRMEL7


3、使用说明
    
    系统配置；
        1、RTC时钟源：LSE
        2、闹钟IO输出：PC13
        3、串口配置：
                            - 串口为USART1（TX：PA9  RX：PA10）:
                            - 数据位：8
                            - 停止位：1
                            - 奇偶校验：无
                            - 波特率： 115200 

    使用方法：
    编译后烧录到评估板，上电后，RTC闹钟每隔500ms产生闹钟中断
    串口会打印:500ms Alarm Wakeup  并且LED1 闪烁。

4、注意事项
    无
	
1. Function description

	1. Trigger the alarm interrupt by setting the alarm time.
	2. Configure I/O output through the alarm flag

2. Use environment

	Software development environment: KEIL MDK-ARM V5.25
	Hardware environment:
		1. based on the evaluation board N32G4FRML-STB V1.1 development
		2. MCU: N32G4FRMEL7

3. Instructions for use

	System configuration:

		1. RTC clock source: LSE
		2. alarm IO output: PC13
		3. Serial port configuration:

							- Serial port: USART1 (TX: PA9 RX: PA10) :
							- Data bit: 8
							- Stop bit: 1
							- Parity check: None
							- Baud rate: 115200

	Instructions:
		After compiling, it is burned to the evaluation board. After powering on, the RTC alarm clock generates alarm interruption every 500ms.
		The serial port will print: 500ms Alarm Wakeup, and LED1 blinking.

4. Matters needing attention
	None
	