1、功能说明

    /* 简单描述工程功能 */
        这个例程配置并演示如何修改线程模式特权访问及堆栈


2、使用环境

    /* 硬件环境：工程对应的开发硬件平台 */
        开发板：N32G4XM-STBV1.1


3、使用说明
    
    /* 描述相关模块配置方法；例如:时钟，I/O等 */
        SystemClock：144MHz
        USART：TX - PA9，RX - PA10，波特率115200

    /* 描述Demo的测试步骤和现象 */
        1.编译后下载程序复位运行；
        2.可使用编译器的“Cortex寄存器”窗口查看线程模式下，使用的堆栈及代码的访问级别（特权级/非特权级）；


4、注意事项


1. Function description
	/* A brief description of the engineering function */
	This routine configudes and demonstrates how to modify thread mode privileged access and stack

2. Use environment
	/* Hardware environment: the corresponding development hardware platform */
	Development board: N32G4XM-STBV1.1

3. Instructions for use    
	/* Describe the related module configuration method; For example: clock, I/O, etc. */
	SystemClock: 144 MHZ
	USART: TX-PA9, RX-PA10, baud rate 115200

	/* Describes the test steps and symptoms of Demo */
	1. Reset and run the downloaded program after compilation;
	2. Use the Compiler's Cortex Register window to view the stack and code access level (privileged/non-privileged) in thread mode.

4. Matters needing attention