1、功能说明

    此例程展示了通过I2C模块与外部EEPRON的通信。   

2、使用环境

   软件开发环境：
        IDE工具：KEIL MDK-ARM 5.34.0.0
	         IAR EWARM 8.50.1
    
    硬件环境：
        开发板：N32A003F5QX-STB V1.0


3、使用说明
	
    1、主时钟：48MHz
    2、I2C 配置：
            SCL   -->  PA4          
            SDA   -->  PA5         
            CLOCK:400KHz
            
    3、UART1配置：
            TX  -->  PA2   
            RX  -->  PA3           
            波特率：115200
    
    4、测试使用EEPROM型号:
	    AT24C04（容量4kb）
        

    5、测试步骤与现象
        a，检查EEPROM连接
        b，编译下载代码复位运行
        c，从串口看打印信息，验证结果

4、注意事项
   无

1. Function description

     This example demonstrates the communication with the external EEPRON through the I2C module.

2. Use environment

    Software development environment:
         IDE tool: KEIL MDK-ARM 5.34.0.0
    
     Hardware environment:
         Development board: N32A003F5QX-STB V1.0


3. Instructions for use

     1. Main clock: 48MHz
     2. I2C configuration:
             SCL --> PA4
             SDA --> PA5
             CLOCK: 400KHz
            
     3. UART1 configuration:
             TX --> PA2
             RX --> PA3
             Baud rate: 115200
    
     4. Test using EEPROM model:
            AT24C04 (capacity 4kb)
        
     5. Test steps and phenomena
         a, check the EEPROM connection
         b, compile and download the code, reset and run
         c, view the print information from the serial port and verify the result

4. Matters needing attention
    without