*PADS-LOGIC-V9.0-CP936* DESIGN EXPORT FILE FROM PADS LOGIC VVX.2.7
*SCH*        GENERAL PARAMETERS OF THE SCHEMATIC DESIGN"

CUR SHEET    1              Current Active Sheet
USERGRID     100    10      Design and Label/Text grid settings
LINEWIDTH    10             Width items will be created with
CONNWIDTH    10             Width used to plot connections
BUSWIDTH     25             Width used to plot buses
BUSANGLE     25             Angle used when plotting buses
NNVISPWRGND  4              Pwr/Gnd netname visibility default flag
PCBFLAGS     1039           PCB Netlist and ECO options
PINNAMESIZE  97     10      Height and LineWidth used by pin names
TEXTSIZE     97     10      Height and LineWidth text will be created width
JOBTIME      0              Amount of time spent on this LOGIC design
DOTGRID      100            Space in thous/inch between graphic dots
BACKUPTIME   5              Number of minutes between database backups
TIEDOTSIZE   75             Diameter of tiedot point
REFNAMESIZE  100    10      Height and LineWidth used by part ref. names
PARTNAMESIZE 100    10      Height and LineWidth used by part type names
PINNOSIZE    97     10      Height and LineWidth used by pin numbers
NETNAMESIZE  100    10      Height and LineWidth used by net names
REAL WIDTH   36             Widths greater then this are displayed real size
SHEET SIZE   A4            
UNITS        0              Rules units type
JOBNAME      N32A003F5QX_STB_V1.0.sch
NTXCOL 11 9
HIRCOL 14
LINCOL 4
TXTCOL 0 15
CONCOL 4
BUSCOL 14
PTXCOL 0 15
COMCOL 9
NMCOL  12 15
PNMCOL 12 15
PINCOL 0 15
NETCOL 1 15
FBGCOL 12 15
OFFREFVIEW   0              Offsheet references visibility default flag
OFFREFNUM    0              Offsheet references per line
SHEETNUMSEP  []             Sheet Number separators
FONT MODE   System
DEFAULT FONT "Regular Tahoma"
BORDER NAME DRW_NATIONS_A4
FIELDCOL 1 15

*CAM* PLOTTER SETTINGS 
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

PLOT_SECTION	5.0
{
PLOT_DEFAULTS_PHOTO_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_MPOS_V1
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Current
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PEN_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_FNT_V0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 Y
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Selected
DEFAULT_SHEET_LIST	NULL
{
SHEET_1	2
SHEET_2	4
SHEET_3	5
SHEET_4	6
SHEET_5	8
SHEET_6	1
SHEET_7	7
}
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PRINTER	NULL
{
DEFAULT_FILE_PREFIX	 NZ3101_FNT_BCM_0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	All
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_AUGMENT_ON_THE_FLY	Y
}

*MISC*      MISCELLANEOUS PARAMETERS
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	MILS
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	Top
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ASSOCIATED_SILK_SCREEN	Silkscreen Top
ASSOCIATED_PASTE_MASK	Paste Mask Top
ASSOCIATED_SOLDER_MASK	Solder Mask Top
ASSOCIATED_ASSEMBLY	Assembly Drawing Top
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	Bottom
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Layer_3
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	4
{
LAYER_NAME	Layer_4
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	Layer_21
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Layer_22
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Layer_23
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	Layer_24
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Layer_26
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	Layer_27
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	Layer_28
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Layer_29
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	Layer_30
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	31
{
LAYER_NAME	Layer_31
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	32
{
LAYER_NAME	Layer_32
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	33
{
LAYER_NAME	Layer_33
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	34
{
LAYER_NAME	Layer_34
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	35
{
LAYER_NAME	Layer_35
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	36
{
LAYER_NAME	Layer_36
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	37
{
LAYER_NAME	Layer_37
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	38
{
LAYER_NAME	Layer_38
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	39
{
LAYER_NAME	Layer_39
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	40
{
LAYER_NAME	Layer_40
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	41
{
LAYER_NAME	Layer_41
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	42
{
LAYER_NAME	Layer_42
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	43
{
LAYER_NAME	Layer_43
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	44
{
LAYER_NAME	Layer_44
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	45
{
LAYER_NAME	Layer_45
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	46
{
LAYER_NAME	Layer_46
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	47
{
LAYER_NAME	Layer_47
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	48
{
LAYER_NAME	Layer_48
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	49
{
LAYER_NAME	Layer_49
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	50
{
LAYER_NAME	Layer_50
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	51
{
LAYER_NAME	Layer_51
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	52
{
LAYER_NAME	Layer_52
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	53
{
LAYER_NAME	Layer_53
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	54
{
LAYER_NAME	Layer_54
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	55
{
LAYER_NAME	Layer_55
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	56
{
LAYER_NAME	Layer_56
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	57
{
LAYER_NAME	Layer_57
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	58
{
LAYER_NAME	Layer_58
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	59
{
LAYER_NAME	Layer_59
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	60
{
LAYER_NAME	Layer_60
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	61
{
LAYER_NAME	Layer_61
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	62
{
LAYER_NAME	Layer_62
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	63
{
LAYER_NAME	Layer_63
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	64
{
LAYER_NAME	Layer_64
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	65
{
LAYER_NAME	Layer_65
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	66
{
LAYER_NAME	Layer_66
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	67
{
LAYER_NAME	Layer_67
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	68
{
LAYER_NAME	Layer_68
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	69
{
LAYER_NAME	Layer_69
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	70
{
LAYER_NAME	Layer_70
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	71
{
LAYER_NAME	Layer_71
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	72
{
LAYER_NAME	Layer_72
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	73
{
LAYER_NAME	Layer_73
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	74
{
LAYER_NAME	Layer_74
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	75
{
LAYER_NAME	Layer_75
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	76
{
LAYER_NAME	Layer_76
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	77
{
LAYER_NAME	Layer_77
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	78
{
LAYER_NAME	Layer_78
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	79
{
LAYER_NAME	Layer_79
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	80
{
LAYER_NAME	Layer_80
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	81
{
LAYER_NAME	Layer_81
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	82
{
LAYER_NAME	Layer_82
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	83
{
LAYER_NAME	Layer_83
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	84
{
LAYER_NAME	Layer_84
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	85
{
LAYER_NAME	Layer_85
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	86
{
LAYER_NAME	Layer_86
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	87
{
LAYER_NAME	Layer_87
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	88
{
LAYER_NAME	Layer_88
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	89
{
LAYER_NAME	Layer_89
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	90
{
LAYER_NAME	Layer_90
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	91
{
LAYER_NAME	Layer_91
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	92
{
LAYER_NAME	Layer_92
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	93
{
LAYER_NAME	Layer_93
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	94
{
LAYER_NAME	Layer_94
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	95
{
LAYER_NAME	Layer_95
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	96
{
LAYER_NAME	Layer_96
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	97
{
LAYER_NAME	Layer_97
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	98
{
LAYER_NAME	Layer_98
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	99
{
LAYER_NAME	Layer_99
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	100
{
LAYER_NAME	Layer_100
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	101
{
LAYER_NAME	Layer_101
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	102
{
LAYER_NAME	Layer_102
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	103
{
LAYER_NAME	Layer_103
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	104
{
LAYER_NAME	Layer_104
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	105
{
LAYER_NAME	Layer_105
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	106
{
LAYER_NAME	Layer_106
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	107
{
LAYER_NAME	Layer_107
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	108
{
LAYER_NAME	Layer_108
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	109
{
LAYER_NAME	Layer_109
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	110
{
LAYER_NAME	Layer_110
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	111
{
LAYER_NAME	Layer_111
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	112
{
LAYER_NAME	Layer_112
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	113
{
LAYER_NAME	Layer_113
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	114
{
LAYER_NAME	Layer_114
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	115
{
LAYER_NAME	Layer_115
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	116
{
LAYER_NAME	Layer_116
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	117
{
LAYER_NAME	Layer_117
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	118
{
LAYER_NAME	Layer_118
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	119
{
LAYER_NAME	Layer_119
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	120
{
LAYER_NAME	Layer_120
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	121
{
LAYER_NAME	Solder Mask Top
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	122
{
LAYER_NAME	Paste Mask Bottom
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	123
{
LAYER_NAME	Paste Mask Top
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	124
{
LAYER_NAME	Drill Drawing
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	125
{
LAYER_NAME	Layer_125
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	126
{
LAYER_NAME	Silkscreen Top
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	127
{
LAYER_NAME	Assembly Drawing Top
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	128
{
LAYER_NAME	Solder Mask Bottom
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	129
{
LAYER_NAME	Silkscreen Bottom
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	130
{
LAYER_NAME	Assembly Drawing Bottom
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	131
{
LAYER_NAME	Layer_131
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	132
{
LAYER_NAME	Layer_132
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	133
{
LAYER_NAME	Layer_133
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	134
{
LAYER_NAME	Layer_134
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	135
{
LAYER_NAME	Layer_135
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	136
{
LAYER_NAME	Layer_136
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	137
{
LAYER_NAME	Layer_137
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	138
{
LAYER_NAME	Layer_138
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	139
{
LAYER_NAME	Layer_139
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	140
{
LAYER_NAME	Layer_140
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	141
{
LAYER_NAME	Layer_141
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	142
{
LAYER_NAME	Layer_142
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	143
{
LAYER_NAME	Layer_143
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	144
{
LAYER_NAME	Layer_144
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	145
{
LAYER_NAME	Layer_145
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	146
{
LAYER_NAME	Layer_146
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	147
{
LAYER_NAME	Layer_147
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	148
{
LAYER_NAME	Layer_148
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	149
{
LAYER_NAME	Layer_149
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	150
{
LAYER_NAME	Layer_150
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	151
{
LAYER_NAME	Layer_151
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	152
{
LAYER_NAME	Layer_152
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	153
{
LAYER_NAME	Layer_153
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	154
{
LAYER_NAME	Layer_154
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	155
{
LAYER_NAME	Layer_155
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	156
{
LAYER_NAME	Layer_156
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	157
{
LAYER_NAME	Layer_157
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	158
{
LAYER_NAME	Layer_158
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	159
{
LAYER_NAME	Layer_159
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	160
{
LAYER_NAME	Layer_160
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	161
{
LAYER_NAME	Layer_161
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	162
{
LAYER_NAME	Layer_162
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	163
{
LAYER_NAME	Layer_163
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	164
{
LAYER_NAME	Layer_164
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	165
{
LAYER_NAME	Layer_165
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	166
{
LAYER_NAME	Layer_166
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	167
{
LAYER_NAME	Layer_167
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	168
{
LAYER_NAME	Layer_168
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	169
{
LAYER_NAME	Layer_169
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	170
{
LAYER_NAME	Layer_170
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	171
{
LAYER_NAME	Layer_171
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	172
{
LAYER_NAME	Layer_172
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	173
{
LAYER_NAME	Layer_173
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	174
{
LAYER_NAME	Layer_174
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	175
{
LAYER_NAME	Layer_175
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	176
{
LAYER_NAME	Layer_176
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	177
{
LAYER_NAME	Layer_177
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	178
{
LAYER_NAME	Layer_178
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	179
{
LAYER_NAME	Layer_179
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	180
{
LAYER_NAME	Layer_180
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	181
{
LAYER_NAME	Layer_181
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	182
{
LAYER_NAME	Layer_182
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	183
{
LAYER_NAME	Layer_183
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	184
{
LAYER_NAME	Layer_184
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	185
{
LAYER_NAME	Layer_185
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	186
{
LAYER_NAME	Layer_186
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	187
{
LAYER_NAME	Layer_187
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	188
{
LAYER_NAME	Layer_188
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	189
{
LAYER_NAME	Layer_189
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	190
{
LAYER_NAME	Layer_190
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	191
{
LAYER_NAME	Layer_191
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	192
{
LAYER_NAME	Layer_192
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	193
{
LAYER_NAME	Layer_193
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	194
{
LAYER_NAME	Layer_194
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	195
{
LAYER_NAME	Layer_195
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	196
{
LAYER_NAME	Layer_196
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	197
{
LAYER_NAME	Layer_197
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	198
{
LAYER_NAME	Layer_198
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	199
{
LAYER_NAME	Layer_199
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	200
{
LAYER_NAME	Layer_200
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	201
{
LAYER_NAME	Layer_201
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	202
{
LAYER_NAME	Layer_202
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	203
{
LAYER_NAME	Layer_203
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	204
{
LAYER_NAME	Layer_204
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	205
{
LAYER_NAME	Layer_205
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	206
{
LAYER_NAME	Layer_206
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	207
{
LAYER_NAME	Layer_207
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	208
{
LAYER_NAME	Layer_208
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	209
{
LAYER_NAME	Layer_209
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	210
{
LAYER_NAME	Layer_210
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	211
{
LAYER_NAME	Layer_211
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	212
{
LAYER_NAME	Layer_212
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	213
{
LAYER_NAME	Layer_213
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	214
{
LAYER_NAME	Layer_214
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	215
{
LAYER_NAME	Layer_215
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	216
{
LAYER_NAME	Layer_216
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	217
{
LAYER_NAME	Layer_217
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	218
{
LAYER_NAME	Layer_218
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	219
{
LAYER_NAME	Layer_219
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	220
{
LAYER_NAME	Layer_220
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	221
{
LAYER_NAME	Layer_221
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	222
{
LAYER_NAME	Layer_222
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	223
{
LAYER_NAME	Layer_223
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	224
{
LAYER_NAME	Layer_224
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	225
{
LAYER_NAME	Layer_225
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	226
{
LAYER_NAME	Layer_226
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	227
{
LAYER_NAME	Layer_227
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	228
{
LAYER_NAME	Layer_228
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	229
{
LAYER_NAME	Layer_229
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	230
{
LAYER_NAME	Layer_230
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	231
{
LAYER_NAME	Layer_231
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	232
{
LAYER_NAME	Layer_232
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	233
{
LAYER_NAME	Layer_233
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	234
{
LAYER_NAME	Layer_234
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	235
{
LAYER_NAME	Layer_235
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	236
{
LAYER_NAME	Layer_236
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	237
{
LAYER_NAME	Layer_237
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	238
{
LAYER_NAME	Layer_238
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	239
{
LAYER_NAME	Layer_239
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	240
{
LAYER_NAME	Layer_240
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	241
{
LAYER_NAME	Layer_241
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	242
{
LAYER_NAME	Layer_242
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	243
{
LAYER_NAME	Layer_243
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	244
{
LAYER_NAME	Layer_244
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	245
{
LAYER_NAME	Layer_245
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	246
{
LAYER_NAME	Layer_246
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	247
{
LAYER_NAME	Layer_247
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	248
{
LAYER_NAME	Layer_248
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	249
{
LAYER_NAME	Layer_249
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	250
{
LAYER_NAME	Layer_250
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	MILS
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	10
COPPER_TO_VIA	10
COPPER_TO_PAD	10
COPPER_TO_SMD	10
COPPER_TO_COPPER	10
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	13
OUTLINE_TO_VIA	13
OUTLINE_TO_PAD	13
OUTLINE_TO_SMD	13
OUTLINE_TO_COPPER	13
DRILL_TO_TRACK	7
DRILL_TO_VIA	7
DRILL_TO_PAD	7
DRILL_TO_SMD	7
DRILL_TO_COPPER	7
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	30
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	50000
STUB_LENGTH	0
PARALLEL_LENGTH	1000
PARALLEL_GAP	200
TANDEM_LENGTH	1000
TANDEM_GAP	200
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	200
MATCH_LENGTH_TOLERANCE	200
}
}
}
}

*FIELDS*    USER FIELDS

"Drawn By" 
"Checked By" 
"QC By" 
"Released By" 
"Drawn Date" 2025-12-15
"Checked Date" 
"QC Date" 
"Release Date" 
"Company Name" Nations
"TITLE" N32A003F5QX-STB
"CODE" 
"Drawing Number" 
"Revision" V1.0
"SCALE" 
"DRAWN" 
"CHECKED" 
"QUALITY CONTROL" 
"RELEASED" 
"COMPANY" 
"COMPANY ADDRESS" 
"DRAWING NO" 
"REV" 

*SHT*   2 NS-LINK -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        6.341          Scale of window expansion
WINDOWCENTER 2782   1790    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

2550   7150   0   1 222  10 0 "Regular Arial Unicode MS"
DEBUG USB
2250   4050   0   1 222  10 0 "Regular Arial Unicode MS"
LED
4850   7150   0   1 222  10 0 "Regular Arial Unicode MS"
MCU
6100   7550   0   1 222  10 0 "Regular Arial Unicode MS"
NS-LINK
4078   1906   0   1 222  10 0 "Regular Arial Unicode MS"
3.3 TO 5V

*LINES*      LINES ITEMS

DRW20918         LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1200  232    0   0 97   10 1 "Regular Arial Unicode MS"
TITLE
-1202  -110   0   0 97   10 1 "Regular Arial Unicode MS"
Drawn Date
-300   42     0   0 97   10 1 "Regular Arial Unicode MS"
Revision
50     774    0   0 250  25 0 "Regular Arial Unicode MS"
A
50     2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
50     4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
50     6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-896   7400   0   0 250  25 0 "Regular Arial Unicode MS"
1
-2680  7400   0   0 250  25 0 "Regular Arial Unicode MS"
2
-4526  7400   0   0 250  25 0 "Regular Arial Unicode MS"
3
-6246  7400   0   0 250  25 0 "Regular Arial Unicode MS"
4
-8026  7400   0   0 250  25 0 "Regular Arial Unicode MS"
5
-9810  7400   0   0 250  25 0 "Regular Arial Unicode MS"
6
-1560  42     0   0 97   10 0 "Regular Arial Unicode MS"
SIZE:
-1560  -110   0   0 97   10 0 "Regular Arial Unicode MS"
DATED:
-10900 2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
-10900 774    0   0 250  25 0 "Regular Arial Unicode MS"
A
-10900 4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
-10900 6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-1102  42     0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Size
-118   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Number of Sheets
-320   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Number
-630   -110   0   0 97   10 0 "Regular Arial Unicode MS"
SHEET:     OF
-630   42     0   0 97   10 0 "Regular Arial Unicode MS"
REV:
-1560  232    0   0 97   10 0 "Regular Arial Unicode MS"
TITLE:
D25057           LINES    3300   7400   1   0
CLOSED 5   10  0  
0      0     
0      -5100 
7400   -5100 
7400   0     
0      0     
D25058           LINES    700    7400   1   0
CLOSED 5   10  0  
0      0     
0      -2900 
2500   -2900 
2500   0     
0      0     
D25059           LINES    6600   2200   1   0
CLOSED 5   10  0  
0      0     
0      -1600 
2600   -1600 
2600   0     
0      0     
D25060           LINES    700    4400   1   0
CLOSED 5   10  0  
0      0     
0      -2100 
2500   -2100 
2500   0     
0      0     
DRW26078         LINES    600    7800   1   0
OPEN   8   10  0  
0      0     
0      -7300 
8800   -7300 
8800   -5600 
10200  -5600 
10200  0     
0      0     
0      -100  
D94437           LINES    700    2200   1   0
CLOSED 5   10  0  
0      0     
0      -1600 
5700   -1600 
5700   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

PIN50            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 1970.01.01.00.00.00
"Default Font"
"Default Font"
-320 300 0 8 107 10 "Default Font"
REF-DES
-550 300 0 1 107 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-100  0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CON_MINIUSB      32000 32000 100 10 100 10 4 1 0 11 0 0
TIMESTAMP 2019.12.11.09.21.40
"Default Font"
"Default Font"
80 1260 0 4 100 10 "Default Font"
REF-DES
290 -40 0 6 100 10 "Default Font"
PART-TYPE
340 -150 0 6 100 10 "Default Font"
*
350 -270 0 6 100 10 "Default Font"
*
OPEN   5   10  255
0     0    
0     1200 
500   1200 
500   0    
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CON-SIP-4P       32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.11.27.05.40.08
"Default Font"
"Default Font"
50 50 0 4 97 10 "Default Font"
REF-DES
100 -500 0 6 97 10 "Default Font"
PART-TYPE
100 -600 0 6 97 10 "Default Font"
*
100 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -500 
200   -500 
200   0    
0     0    
T-100  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -200  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -300  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -400  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

DIODE            32000 32000 90 10 80 10 4 4 0 2 18 0
TIMESTAMP 2019.12.01.15.48.44
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0

CON1X3           32000 32000 100 10 100 10 4 7 0 3 0 0
TIMESTAMP 2019.12.01.16.15.06
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 -250 0 6 100 10 "Default Font"
PART-TYPE
0 -240 0 6 100 10 "Default Font"
*
0 -340 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
0     50   
0     150  
CIRCLE 2   10  255
0     -50  
0     50   
CLOSED 5   10  255
-100  200  
-100  -200 
100   -200 
100   200  
-100  200  
CIRCLE 2   10  255
0     -50  
0     -150 
OPEN   2   10  255
-100  100  
-50   100  
OPEN   2   10  255
-100  -100 
-50   -100 
OPEN   2   10  255
-50   0    
-100  0    
T-200  100   0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

RES0402          32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2022.10.25.06.30.33
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CAP0603          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.25.06.24.16
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CAP0402          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.25.06.23.43
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CAP0805          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.24.07.07.40
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

LQFP48           32000 32000 97 10 97 10 4 1 0 48 0 0
TIMESTAMP 2022.10.24.07.55.59
"Default Font"
"Default Font"
2300 2340 0 0 97 10 "Default Font"
REF-DES
2300 -40 0 2 97 10 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 "Default Font"
*
2300 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2300  0    
2300  2300 
0     2300 
0     0    
T-200  1700  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1700  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

TXS0104EPWR      32000 32000 100 10 100 10 2 3 0 14 3 0
TIMESTAMP 1970.01.01.00.00.00
"Default Font"
"Default Font"
0 0 0 0 100 10 "Regular default"
REF-DES
0 0 0 0 100 10 "Default Font"
PART-TYPE
CIRCLE 2   10  255
-360  370  
-340  370  
CIRCLE 2   10  255
-360  370  
-340  370  
CLOSED 5   10  255
-400  -420 
-400  420  
400   420  
400   -420 
-400  -420 
T-500  300   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  200   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  100   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  0     0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -100  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -200  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -300  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -300  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -200  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -100  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   0     0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   100   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   200   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   300   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2019.11.20.07.32.26
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

RES              32000 32000 100 10 100 10 4 1 0 2 26 0
TIMESTAMP 2023.10.19.06.35.11
"Default Font"
"Default Font"
0 0 0 4 70 7 "Default Font"
REF-DES
240 -110 0 6 70 7 "Default Font"
PART-TYPE
150 30 0 6 70 7 "Default Font"
VALUE
210 -170 0 6 70 7 "Default Font"
*
CLOSED 5   10  255
50    -40  
50    40   
250   40   
250   -40  
50    -40  
T0     0     0 0 20 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T300   0     0 1 0 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

MINIUSB CON  1   0   0     0
TIMESTAMP 2019.12.11.09.21.39
GATE 1 11 0
CON_MINIUSB
1 0 U VBUS
2 0 U D-
3 0 U D+
4 0 U ID
5 0 U GND
6 0 U SHIELD1
7 0 U SHIELD2
8 0 U SHIELD3
9 0 U SHIELD4
10 0 U H1
11 0 U H2

CON-SIP-4P CON  1   0   0     0
TIMESTAMP 2019.11.27.05.40.07
GATE 1 4 0
CON-SIP-4P
1 0 U
2 0 U
3 0 U
4 0 U

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

DIODE_2 UND  1   0   0     0
TIMESTAMP 2019.12.01.15.48.43
GATE 1 2 0
DIODE
1 0 U
2 0 U

CON1X3 CON  1   0   0     3
TIMESTAMP 2019.12.01.16.15.04
GATE 1 3 0
CON1X3
1 0 U
2 0 U
3 0 U
1 2 3 

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U

RES0402 RES  1   0   0     0
TIMESTAMP 2022.10.25.06.30.33
GATE 1 2 0
RES0402
1 0 U
2 0 U

CAP0603 CAP  1   0   0     0
TIMESTAMP 2022.10.25.06.24.15
GATE 1 2 0
CAP0603
1 1 U
2 1 U

CAP0402 CAP  1   0   0     0
TIMESTAMP 2022.10.25.06.23.42
GATE 1 2 0
CAP0402
1 1 U
2 1 U

CAP0805 CAP  1   0   0     0
TIMESTAMP 2022.10.24.07.07.39
GATE 1 2 0
CAP0805
1 1 U
2 1 U

N32G452CCL7 UND  1   0   0     0
TIMESTAMP 2022.10.24.07.55.59
GATE 1 48 0
LQFP48
1 0 U VBAT
2 0 U PC13-TAMPER-RTC
3 0 U PC14-OSC32_IN
4 0 U PC15-OSC32_OUT
5 0 U PD0-OSC_IN
6 0 U PD1-OSC_OUT
7 0 U NRST
8 0 U VSSA
9 0 U VDDA
10 0 U PA0-WKUP
11 0 U PA1
12 0 U PA2
13 0 U PA3
14 0 U PA4
15 0 U PA5
16 0 U PA6
17 0 U PA7
18 0 U PB0
19 0 U PB1
20 0 U PB2-BOOT
21 0 U PB10
22 0 U PB11
23 0 U VSS_1
24 0 U VDD_1
25 0 U PB12
26 0 U PB13
27 0 U PB14
28 0 U PB15
29 0 U PA8
30 0 U PA9
31 0 U PA10
32 0 U PA11
33 0 U PA12
34 0 U PA13-SWDIO
35 0 U VSS_2
36 0 U VDD_2
37 0 U PA14-SWCLK
38 0 U PA15
39 0 U PB3
40 0 U PB4
41 0 U PB5
42 0 U PB6
43 0 U PB7
44 0 U BOOT0
45 0 U PB8
46 0 U PB9
47 0 U VSS_3
48 0 U VDD_3

TXS0104EPWR TTL  1   0   0     0
TIMESTAMP 1970.01.01.00.00.00
GATE 1 14 0
TXS0104EPWR
1 0 L VCCA
2 0 L A1
3 0 L A2
4 0 L A3
5 0 L A4
6 0 L NC
7 0 L GND
8 0 L OE
9 0 L NC
10 0 L B4
11 0 L B3
12 0 L B2
13 0 L B1
14 0 L VCCB

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2019.11.20.07.32.25
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

RES0402-4.7K RES  1   0   0     0
TIMESTAMP 2012.09.11.08.57.54
GATE 1 2 0
RES
1 0 U
2 0 U



*PART*       ITEMS



J4           MINIUSB          1350  5150    0 1 97 10 97 10 4 3 11 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 1300 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
290 -40 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
340 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
350 -270 0 6 97 10 0 "Regular Arial Unicode MS"
*
"DECAL" 
"Description" 6 pin header
"PCB DECAL" CON_MINIUSB
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1

J10          CON-SIP-4P       8400  1600    0 0 97 10 97 10 4 1 4 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 50 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
100 -500 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -600 0 6 97 10 0 "Regular Arial Unicode MS"
*
100 -700 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SIP-4P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1
3 60 10 0 1

R20          RES0402          2750  3650    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
110 110 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-100 130 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R15          RES0402          2750  3050    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
110 120 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-90 160 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

D6           LED0805          1850  3700    0 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
300 -200 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D7           LED0805          1850  3100    0 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
300 -200 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D5           DIODE_2          2050  6400    0 0 97 10 97 10 4 2 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 150 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
300 -150 0 6 97 10 1 "Regular Arial Unicode MS"
VALUE
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SOD123
"VALUE" SS14L
0 130 14 0 1
1 130 14 0 1

R11          RES0402          1850  6100    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
80 120 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
280 140 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R12          RES0402          1850  6000    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
70 -80 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
280 30 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

C22          CAP0805          1800  6850    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
180 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
180 -250 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" CAP0805
0 20 -80 0 0
1 20 -80 0 0

U4           N32G452CCL7      6400  3400    0 0 97 10 97 10 4 2 48 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
1130 1340 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
2300 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
920 1210 0 2 97 10 1 "Regular Arial Unicode MS"
Value
2300 -240 0 2 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" NS-LQFP48-50P900X900X160
"Value" N32G452CCL7
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

C30          CAP0402          4080  5400   90 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C32          CAP0402          4100  4600   90 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

R19          RES0402          9000  4050    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
60 140 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
260 180 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 100R
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R17          RES0402          7650  2750   90 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
230 180 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-40 190 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R4           R0402            4750  4050    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -10 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R18          RES0402          7350  6400   90 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
190 -70 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-10 -80 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

C5           CAP0402          5350  5350    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-130 -130 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-210 -360 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C9           CAP0402          5500  4200    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C14          CAP0402          8300  3100    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C18          CAP0402          9200  5600    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C19          CAP0603          6000  5800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-170 -150 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-210 -360 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" CAP0603
0 20 -90 0 0
1 20 -80 0 0

C20          CAP0402          6300  5800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-200 -160 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-230 -350 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

R24          R0402            6050  4150    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 0 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J12          CON1X3           5900  6900    0 1 97 10 97 10 4 2 3 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 250 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -250 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -240 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -340 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Marking" 
"PCB DECAL" 2.54MM_CON3P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1

C1           CAP0402          5000  3900    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

Y1           CRYSTAL_2PIN     4700  5250   90 3 97 10 97 10 4 2 2 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 -200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
260 -120 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
350 -200 90 5 97 10 1 "Regular Arial Unicode MS"
Value
240 -396 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Value" 8MHz
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1

U3           TXS0104EPWR      3700  1300    0 0 97 10 97 10 23 22 14 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-54 -524 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
-302 -654 0 0 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 0 0 0 97 10 0 "Default Font"
Comment
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Symbol
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Device
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
LCSC_Part_Name
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier_Part
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Manufacturer
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Manufacturer_Part
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier_Footprint
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
JLCPCB_Part_Class
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Datasheet
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Add_into_BOM
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Convert_to_PCB
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Channel_Type
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Data_Rate
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Voltage___Supply(VCCA)
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Voltage___Supply(VCCB)
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Number_of_Circuits
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Output_Type
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Operating_Temperature
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Features
"Comment" TXS0104EPWR
"Symbol" TXS0104EPWR
"Device" TXS0104EPWR
"LCSC_Part_Name" TXS0104EPWR
"Supplier_Part" C44955
"Manufacturer" 
"Manufacturer_Part" TXS0104EPWR
"Supplier_Footprint" TSSOP-14
"JLCPCB_Part_Class" Extended Part
"Datasheet" https://www.ti.com/cn/lit/gpn/txs0104e
"Supplier" LCSC
"Add_into_BOM" yes
"Convert_to_PCB" yes
"Channel_Type" 
"Data_Rate" 24Mbps
"Voltage___Supply(VCCA)" 1.65V~3.6V
"Voltage___Supply(VCCB)" 2.3V~5.5V
"Number_of_Circuits" 4
"Output_Type" 
"Operating_Temperature" 
"Features" 
"PCB DECAL" TSSOP-14_L5.0-W4.4-P0.65-LS6.4-BL
0 50 0 0 0
1 50 0 0 0
2 50 0 0 0
3 50 0 0 0
4 50 0 0 0
5 50 0 0 0
6 50 0 0 0
7 50 0 0 0
8 50 0 0 0
9 50 0 0 0
10 50 0 0 0
11 50 0 0 0
12 50 0 0 0
13 50 0 0 0

J19          CONDIP2_A        4950  1500   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J20          CONDIP2_A        4950  1400   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J21          CONDIP2_A        4950  1300   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J22          CONDIP2_A        4950  1200   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R27          RES0402-4.7K     4804  998     0 1 97 10 97 10 4 7 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
222 -154 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
240 -110 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
-6 -90 0 6 97 7 3 "Default Font"
Value
210 -170 0 6 97 7 0 "Regular Arial Unicode MS"
*
"Code" 045020100277
"Description" RC0402FR-074K7L(4.7k¦¸,¡À1%,1/16W,SMD0402,YAGEO)
"Manufacturer" YAGEO
"PACKAGE" RES0402
"Part Number" RC0402FR-074K7L
"Value" 4.7K
"PCB DECAL" RES0402
0 20 20 0 0
1 0 20 0 0

J5           CONDIP2_A        7100  2700   90 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-90 10 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 1800   6850   0 3 0
@@@O1    DP_NSLINK $OSR_SYMS 2350   6050   0 1 0
@@@O2    DM_NSLINK $OSR_SYMS 2350   6150   0 1 0
@@@O3    GND $GND_SYMS 1750   5450   0 0 0
@@@O4    GND $GND_SYMS 3000   3050   0 0 0
@@@O5    LED_CON/PB6 $OSR_SYMS 1750   3700   0 0 0
@@@O6    LED_RUN/PA8 $OSR_SYMS 1750   3100   0 0 0
@@@O7    5V $PWR_SYMS 2750   6450   0 0 0
@@@O8    VDD_LINK $PWR_SYMS 8150   1600   0 0 0
@@@O9    PA13/TMS/SWDIO $OSR_SYMS 8100   1400   0 0 0
@@@O10   PA14/TCK/SWCLK $OSR_SYMS 8100   1300   0 0 0
@@@O11   GND $GND_SYMS 8150   1150   0 0 0
@@@O12   VDD_LINK $PWR_SYMS 4300   4100   90 0 0
@@@O13   GND $GND_SYMS 5000   3350   0 0 0
@@@O14   DM_NSLINK $OSR_SYMS 9450   4700   0 1 0
@@@O15   DP_NSLINK $OSR_SYMS 9450   4800   0 1 0
@@@O16   PA0 $OSR_SYMS 6900   2700   0 0 0
@@@O17   PA14/TCK/SWCLK $OSR_SYMS 8100   6000   90 2 0
@@@O18   PA13/TMS/SWDIO $OSR_SYMS 9450   4900   0 1 0
@@@O19   LED_RUN/PA8 $OSR_SYMS 9450   4400   0 1 0
@@@O20   LED_CON/PB6 $OSR_SYMS 7600   6000   90 2 0
@@@O21   GND $GND_SYMS 7700   2600   0 0 0
@@@O22   VDD_LINK $PWR_SYMS 5600   5800   0 0 0
@@@O23   VDD_LINK $PWR_SYMS 7000   6450   0 0 0
@@@O24   VDD_LINK $PWR_SYMS 9000   5800   0 0 0
@@@O25   GND $GND_SYMS 9250   5000   90 0 0
@@@O26   GND $GND_SYMS 7100   6100   0 2 0
@@@O27   GND $GND_SYMS 8000   3000   0 0 0
@@@O28   VDD_LINK $PWR_SYMS 8550   3100   90 1 0
@@@O29   NSLINK_TCK_SWCLK $OSR_SYMS 9450   4100   0 1 0
@@@O30   NSLINK_TMS_SWDIO $OSR_SYMS 9450   4200   0 1 0
@@@O31   GND $GND_SYMS 4050   4600   90 1 0
@@@O32   GND $GND_SYMS 4050   5400   90 1 0
@@@O33   GND $GND_SYMS 6200   4400   90 1 0
@@@O34   VDD_LINK $PWR_SYMS 6150   7000   90 1 0
@@@O35   GND $GND_SYMS 6200   6800   90 0 0
@@@O36   NSLINK_USART1_RX $OSR_SYMS 9450   4600   0 1 0
@@@O37   NSLINK_USART1_TX $OSR_SYMS 9450   4500   0 1 0
@@@O38   GND $GND_SYMS 6200   5700   0 0 0
@@@O39   GND $GND_SYMS 5350   4900   0 0 0
@@@O40   GND $GND_SYMS 5500   3450   0 0 0
@@@O41   GND $GND_SYMS 8300   2600   0 0 0
@@@O42   VDD_LINK $PWR_SYMS 2700   1800   0 0 0
@@@O43   VDD_MCU $PWR_SYMS 4750   1800   0 0 0
@@@O44   NSLINK_USART1_RX $OSR_SYMS 2300   1500   0 0 0
@@@O45   NSLINK_USART1_TX $OSR_SYMS 2300   1400   0 0 0
@@@O46   NSLINK_TMS_SWDIO $OSR_SYMS 2300   1300   0 0 0
@@@O47   NSLINK_TCK_SWCLK $OSR_SYMS 2300   1200   0 0 0
@@@O48   PA2/TX1 $OSR_SYMS 5400   1500   0 1 0
@@@O49   PA3/RX1 $OSR_SYMS 5400   1400   0 1 0
@@@O50   PA8/SWDIO $OSR_SYMS 5400   1300   0 1 0
@@@O51   PA9/SWDCK $OSR_SYMS 5400   1200   0 1 0
@@@O52   GND $GND_SYMS 2900   950    0 0 0
@@@O53   VDD_LINK $PWR_SYMS 4982   998    90 1 0

*TIEDOTS*



@@@D0    1750   5750  
@@@D1    1750   5650  
@@@D2    1750   5550  
@@@D3    1750   5450  
@@@D4    1800   6400  
@@@D5    3000   3100  
@@@D6    5000   4100  
@@@D7    9350   4200  
@@@D8    4700   5400  
@@@D9    4700   4600  
@@@D10   5600   4300  
@@@D11   5600   5100  
@@@D12   6200   5700  
@@@D13   7000   6400  
@@@D14   6300   6400  
@@@D15   5600   5550  
@@@D16   5600   4300  
@@@D17   8300   3100  
@@@D18   9000   5700  
@@@D19   9200   5000  

*CONNECTION*


*SIGNAL* PA8/SWDIO 0 0
J21.1        @@@O50       2 0
5150   1300  
5400   1300  

*SIGNAL* PA2/TX1 0 0
J19.1        @@@O48       2 0
5150   1500  
5400   1500  

*SIGNAL* PA9/SWDCK 0 0
J22.1        @@@O51       2 0
5150   1200  
5400   1200  

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
U3.14        @@@O43       3 0
4200   1600  
4750   1600  
4750   1800  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        C22.1        2 0
1800   6850  
1800   6850  
J4.5         @@@D0        3 0
1550   5850  
1750   5850  
1750   5750  
J4.6         @@@D0        2 0
1550   5750  
1750   5750  
@@@D0        @@@D1        2 0
1750   5750  
1750   5650  
J4.7         @@@D1        2 0
1550   5650  
1750   5650  
@@@D1        @@@D2        2 0
1750   5650  
1750   5550  
J4.8         @@@D2        2 0
1550   5550  
1750   5550  
@@@D2        @@@D3        2 0
1750   5550  
1750   5450  
J4.9         @@@D3        2 0
1550   5450  
1750   5450  
@@@D3        @@@O3        2 0
1750   5450  
1750   5450  
@@@D5        R20.1        3 0
3000   3100  
3000   3700  
2850   3700  
@@@D5        R15.1        2 0
3000   3100  
2850   3100  
@@@D5        @@@O4        2 0
3000   3100  
3000   3050  
J10.4        @@@O11       3 0
8300   1200  
8150   1200  
8150   1150  
C1.2         @@@O13       2 0
5000   3400  
5000   3350  
@@@O21       R17.1        2 0
7700   2600  
7700   2650  
U4.35        @@@D19       2 0
8900   5000  
9200   5000  
U4.47        @@@O26       2 0
7100   5900  
7100   6100  
@@@O31       C32.1        2 0
4050   4600  
4100   4600  
C30.1        @@@O32       2 0
4080   5400  
4050   5400  
U4.8         @@@O33       2 0
6200   4400  
6200   4400  
U4.23        @@@O27       2 0
8000   3200  
8000   3000  
J12.3        @@@O35       2 0
6100   6800  
6200   6800  
C20.1        @@@D12       3 0
6300   5800  
6300   5700  
6200   5700  
@@@D12       C19.1        3 0
6200   5700  
6000   5700  
6000   5800  
@@@D12       @@@O38       2 0
6200   5700  
6200   5700  
C5.2         @@@O39       2 0
5350   4850  
5350   4900  
C9.2         @@@O40       2 0
5500   3700  
5500   3450  
C14.2        @@@O41       2 0
8300   2600  
8300   2600  
C18.2        @@@D19       2 0
9200   5100  
9200   5000  
@@@D19       @@@O25       2 0
9200   5000  
9250   5000  
U3.7         @@@O52       3 0
3200   1000  
2900   1000  
2900   950   

*SIGNAL* PA0 0 0
J5.1         @@@O16       2 0
6900   2700  
6900   2700  

*SIGNAL* 5V 0 0
D5.1         @@@O7        3 0
2550   6400  
2750   6400  
2750   6450  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J10.1        @@@O8        3 0
8300   1500  
8150   1500  
8150   1600  
@@@O12       R4.2         2 0
4300   4100  
4450   4100  
U4.9         @@@D10       2 0
6200   4300  
5600   4300  
@@@O22       @@@D15       2 0
5600   5800  
5600   5550  
@@@O23       @@@D13       2 0
7000   6450  
7000   6400  
@@@D18       @@@O24       2 0
9000   5700  
9000   5800  
C14.1        @@@D17       2 0
8300   3100  
8300   3100  
@@@D10       R24.2        3 0
5600   4300  
5600   4200  
5750   4200  
@@@D11       @@@D16       2 0
5600   5100  
5600   4300  
@@@D11       U4.1         2 0
5600   5100  
6200   5100  
J12.1        @@@O34       2 0
6100   7000  
6150   7000  
@@@D13       @@@D14       2 0
7000   6400  
6300   6400  
C20.2        @@@D14       2 0
6300   6300  
6300   6400  
@@@D13       U4.48        2 0
7000   6400  
7000   5900  
@@@D14       C19.2        3 0
6300   6400  
6000   6400  
6000   6300  
C5.1         @@@D15       3 0
5350   5350  
5350   5550  
5600   5550  
@@@D15       @@@D11       2 0
5600   5550  
5600   5100  
C9.1         @@@D16       3 0
5500   4200  
5500   4300  
5600   4300  
@@@D16       @@@D10       2 0
5600   4300  
5600   4300  
U4.24        @@@D17       3 0
8100   3200  
8100   3100  
8300   3100  
@@@D17       @@@O28       2 0
8300   3100  
8550   3100  
@@@D18       U4.36        3 0
9000   5700  
9000   5100  
8900   5100  
@@@D18       C18.1        3 0
9000   5700  
9200   5700  
9200   5600  
U3.1         @@@O42       3 0
3200   1600  
2700   1600  
2700   1800  
R27.1        @@@O53       2 0
4804   998   
4982   998   

*SIGNAL* $$$4465 64 0
C22.2        @@@D4        2 0
1800   6350  
1800   6400  
@@@D4        J4.1         3 0
1800   6400  
1800   6250  
1550   6250  
@@@D4        D5.2         2 0
1800   6400  
2050   6400  

*SIGNAL* DM_NSLINK 0 0
R11.2        @@@O2        2 0
2150   6150  
2350   6150  
U4.32        @@@O14       2 0
8900   4700  
9450   4700  

*SIGNAL* DP_NSLINK 0 0
R12.2        @@@O1        2 0
2150   6050  
2350   6050  
U4.33        @@@O15       2 0
8900   4800  
9450   4800  

*SIGNAL* $$$24935 64 0
J4.2         R11.1        2 0
1550   6150  
1750   6150  

*SIGNAL* $$$24997 64 0
J4.3         R12.1        2 0
1550   6050  
1750   6050  

*SIGNAL* $$$32273 64 0
D6.1         R20.2        2 0
2350   3700  
2450   3700  

*SIGNAL* $$$32275 64 0
D7.1         R15.2        2 0
2350   3100  
2450   3100  

*SIGNAL* LED_CON/PB6 0 0
D6.2         @@@O5        2 0
1850   3700  
1750   3700  
U4.42        @@@O20       2 0
7600   5900  
7600   6000  

*SIGNAL* LED_RUN/PA8 0 0
D7.2         @@@O6        2 0
1850   3100  
1750   3100  
@@@O19       U4.29        2 0
9450   4400  
8900   4400  

*SIGNAL* PA13/TMS/SWDIO 0 0
J10.2        @@@O9        2 0
8300   1400  
8100   1400  
U4.34        @@@O18       2 0
8900   4900  
9450   4900  

*SIGNAL* PA14/TCK/SWCLK 0 0
J10.3        @@@O10       2 0
8300   1300  
8100   1300  
U4.37        @@@O17       2 0
8100   5900  
8100   6000  

*SIGNAL* NSLINK_TMS_SWDIO 0 0
@@@D7        U4.27        2 0
9350   4200  
8900   4200  
R19.2        @@@D7        3 0
9300   4000  
9350   4000  
9350   4200  
@@@D7        @@@O30       2 0
9350   4200  
9450   4200  
@@@O46       U3.4         2 0
2300   1300  
3200   1300  

*SIGNAL* NSLINK_TCK_SWCLK 0 0
@@@O29       U4.26        2 0
9450   4100  
8900   4100  
U3.5         @@@O47       2 0
3200   1200  
2300   1200  

*SIGNAL* NSLINK_USART1_TX 0 0
U4.30        @@@O37       2 0
8900   4500  
9450   4500  
@@@O45       U3.3         2 0
2300   1400  
3200   1400  

*SIGNAL* NSLINK_USART1_RX 0 0
U4.31        @@@O36       2 0
8900   4600  
9450   4600  
@@@O44       U3.2         2 0
2300   1500  
3200   1500  

*SIGNAL* $$$14362 64 0
R4.1         @@@D6        2 0
4850   4100  
5000   4100  
@@@D6        U4.7         4 0
5000   4100  
5300   4100  
5300   4500  
6200   4500  
@@@D6        C1.1         2 0
5000   4100  
5000   3900  

*SIGNAL* $$$32474 64 0
R17.2        U4.20        2 0
7700   3050  
7700   3200  

*SIGNAL* $$$32494 64 0
U4.44        R18.1        2 0
7400   5900  
7400   6300  

*SIGNAL* $$$29264 64 0
R18.2        J12.2        3 0
7400   6700  
7400   6900  
6100   6900  

*SIGNAL* $$$18547 64 0
U4.25        R19.1        2 0
8900   4000  
8900   4000  

*SIGNAL* $$$26932 64 0
Y1.2         @@@D9        2 0
4700   4698  
4700   4600  
U4.6         @@@D9        2 0
6200   4600  
4700   4600  
@@@D9        C32.2        2 0
4700   4600  
4600   4600  

*SIGNAL* $$$26931 64 0
Y1.1         @@@D8        2 0
4700   5298  
4700   5400  
U4.5         @@@D8        4 0
6200   4700  
5100   4700  
5100   5400  
4700   5400  
@@@D8        C30.2        2 0
4700   5400  
4580   5400  

*SIGNAL* $$$3902 64 0
U4.10        R24.1        2 0
6200   4200  
6150   4200  

*SIGNAL* PA3/RX1 0 0
J20.1        @@@O49       2 0
5150   1400  
5400   1400  

*SIGNAL* $$$28647 64 0
J22.2        U3.10        2 0
4750   1200  
4200   1200  

*SIGNAL* $$$28650 64 0
U3.11        J21.2        2 0
4200   1300  
4750   1300  

*SIGNAL* $$$28651 64 0
U3.12        J20.2        2 0
4200   1400  
4750   1400  

*SIGNAL* $$$28652 64 0
U3.13        J19.2        2 0
4200   1500  
4750   1500  

*SIGNAL* $$$32065 64 0
U3.8         R27.2        3 0
4200   1000  
4504   1000  
4504   998   

*SIGNAL* $$$26041 64 0
U4.18        J5.2         3 0
7500   3200  
7500   2700  
7300   2700  

*NETNAMES*



DP_NSLINK    @@@O1        320    -40    0 0 0      0      0 3 -1 12 97 "Regular Arial Unicode MS"
DM_NSLINK    @@@O2        322    -32    0 0 0      0      0 3 -1 12 97 "Regular Arial Unicode MS"
LED_CON/PB6  @@@O5        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_RUN/PA8  @@@O6        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
5V           @@@O7        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O8        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA13/TMS/SWDIO @@@O9        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/TCK/SWCLK @@@O10       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O12       -400   0      0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
DM_NSLINK    @@@O14       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
DP_NSLINK    @@@O15       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O16       -330   0      0 9 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA14/TCK/SWCLK @@@O17       -50    950    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA13/TMS/SWDIO @@@O18       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_RUN/PA8  @@@O19       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_CON/PB6  @@@O20       -50    850    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O22       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O23       -300   100    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O24       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O28       400    50     0 7 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TCK_SWCLK @@@O29       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TMS_SWDIO @@@O30       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O34       400    0      0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_RX @@@O36       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_TX @@@O37       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O42       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O43       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_RX @@@O44       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_TX @@@O45       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TMS_SWDIO @@@O46       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TCK_SWCLK @@@O47       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2/TX1      @@@O48       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3/RX1      @@@O49       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA8/SWDIO    @@@O50       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA9/SWDCK    @@@O51       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O53       420    -42    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"

*SHT*   1 MCU -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        5.702          Scale of window expansion
WINDOWCENTER 3532   983     Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

9614   4006   0   0 222  10 0 "Regular Arial Unicode MS"
RESET
7098   4006   0   0 222  10 0 "Regular Arial Unicode MS"
MCU WAKEUP
7700   7508   0   1 222  10 0 "Regular Arial Unicode MS"
KEY
10080  7508   0   1 222  10 0 "Regular Arial Unicode MS"
LED
3600   7508   0   1 222  10 0 "Regular Arial Unicode MS"
LDO
3650   5530   0   1 222  10 0 "Regular Arial Unicode MS"
MCU

*LINES*      LINES ITEMS

DRW_NATIONS_A4   LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1202  -110   0   0 97   10 1 "Regular Arial Unicode MS"
Drawn Date
-1200  232    0   0 97   10 1 "Regular Arial Unicode MS"
TITLE
-1560  232    0   0 97   10 0 "Regular Arial Unicode MS"
TITLE:
-630   42     0   0 97   10 0 "Regular Arial Unicode MS"
REV:
-630   -110   0   0 97   10 0 "Regular Arial Unicode MS"
SHEET:     OF
-320   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Number
-118   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Number of Sheets
-1102  42     0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Size
-300   42     0   0 97   10 1 "Regular Arial Unicode MS"
Revision
-10900 6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-10900 4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
-10900 774    0   0 250  25 0 "Regular Arial Unicode MS"
A
-10900 2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
-1560  -110   0   0 97   10 0 "Regular Arial Unicode MS"
DATED:
-1560  42     0   0 97   10 0 "Regular Arial Unicode MS"
SIZE:
-9810  7400   0   0 250  25 0 "Regular Arial Unicode MS"
6
-8026  7400   0   0 250  25 0 "Regular Arial Unicode MS"
5
-6246  7400   0   0 250  25 0 "Regular Arial Unicode MS"
4
-4526  7400   0   0 250  25 0 "Regular Arial Unicode MS"
3
-2680  7400   0   0 250  25 0 "Regular Arial Unicode MS"
2
-896   7400   0   0 250  25 0 "Regular Arial Unicode MS"
1
50     6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
50     4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
50     2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
50     774    0   0 250  25 0 "Regular Arial Unicode MS"
A
D22894           LINES    8700   4700   1   0
CLOSED 5   10  0  
0      0     
0      -3200 
2400   -3200 
2400   0     
0      0     
D22895           LINES    6500   4700   1   0
CLOSED 5   10  0  
0      0     
0      -3200 
2100   -3200 
2100   0     
0      0     
D23128           LINES    6500   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2100   -3000 
2100   0     
0      0     
D23129           LINES    8700   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2400   -3000 
2400   0     
0      0     
D24779           LINES    600    5800   1   0
CLOSED 5   10  0  
0      0     
0      -5300 
5800   -5300 
5800   0     
0      0     
D24819           LINES    600    7800   1   0
CLOSED 5   10  0  
0      0     
0      -1900 
5800   -1900 
5800   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2020.05.30.04.20.05
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

SPX1117-3V3      32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.12.11.09.57.22
"Default Font"
"Default Font"
200 100 0 4 97 10 "Default Font"
REF-DES
200 -500 0 6 97 10 "Default Font"
PART-TYPE
200 -600 0 6 97 10 "Default Font"
*
200 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -400 
400   -400 
400   0    
0     0    
T-200  -300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

SW_2P            32000 32000 97 10 97 10 4 6 0 2 16 0
TIMESTAMP 2019.01.05.10.52.59
"Default Font"
"Default Font"
0 100 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
0 -200 0 6 97 10 "Default Font"
*
0 -300 0 6 97 10 "Default Font"
*
OPEN   2   20  255
-150  40   
150   40   
OPEN   2   30  255
-80   60   
80    60   
CIRCLE 2   10  255
-60   0    
-100  0    
CIRCLE 2   10  255
100   0    
60    0    
OPEN   2   10  255
80    0    
200   0    
OPEN   2   10  255
-80   0    
-200  0    
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T200   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CAP0805          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.24.07.07.40
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

CAP0402          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.25.06.23.43
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

RES0402          32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2022.10.25.06.30.33
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

HEAD2X16         32000 32000 97 10 97 10 4 1 0 32 0 0
TIMESTAMP 2022.10.25.06.35.56
"Default Font"
"Default Font"
200 1740 0 4 97 10 "Default Font"
REF-DES
750 60 0 6 97 10 "Default Font"
PART-TYPE
750 -40 0 6 97 10 "Default Font"
*
750 -140 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
200   0    
200   1700 
0     1700 
0     0    
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAP0603          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2022.10.25.06.24.16
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

N32A003F5Q7      32000 32000 97 10 97 10 4 1 0 21 0 0
TIMESTAMP 2026.01.13.09.43.27
"Default Font"
"Default Font"
1200 1240 0 0 97 10 "Default Font"
REF-DES
1200 -40 0 2 97 10 "Default Font"
PART-TYPE
1200 -140 0 2 97 10 "Default Font"
*
1200 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
1200  0    
1200  1200 
0     1200 
0     0    
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T300   1400  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2020.05.30.04.20.03
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

AMS1117-3.3 UND  1   0   0     0
TIMESTAMP 2019.12.11.09.57.22
GATE 1 4 0
SPX1117-3V3
1 0 U GND
2 0 U OUT
3 0 U IN
4 0 U OUT

SW_2P UND  1   0   0     2
TIMESTAMP 2019.01.05.10.52.56
GATE 1 2 0
SW_2P
1 0 U
2 0 U
1 2 

CAP0805 CAP  1   0   0     0
TIMESTAMP 2022.10.24.07.07.39
GATE 1 2 0
CAP0805
1 1 U
2 1 U

CAP0402 CAP  1   0   0     0
TIMESTAMP 2022.10.25.06.23.42
GATE 1 2 0
CAP0402
1 1 U
2 1 U

RES0402 RES  1   0   0     0
TIMESTAMP 2022.10.25.06.30.33
GATE 1 2 0
RES0402
1 0 U
2 0 U

HEAD2X16 UND  1   0   0     0
TIMESTAMP 2022.10.25.06.35.54
GATE 1 32 0
HEAD2X16
1 0 L
2 0 L
3 0 L
4 0 L
5 0 L
6 0 L
7 0 L
8 0 L
9 0 L
10 0 L
11 0 L
12 0 L
13 0 L
14 0 L
15 0 L
16 0 L
17 0 L
18 0 L
19 0 L
20 0 L
21 0 U
23 0 U
25 0 U
27 0 U
29 0 U
31 0 U
22 0 U
24 0 U
26 0 U
28 0 U
30 0 U
32 0 U

CAP0603 CAP  1   0   0     0
TIMESTAMP 2022.10.25.06.24.15
GATE 1 2 0
CAP0603
1 1 U
2 1 U

N32A003F5Q7 UND  1   0   0     0
TIMESTAMP 2026.01.13.09.43.27
GATE 1 21 0
N32A003F5Q7
1 0 U PA0/NRST
2 0 U PA1
3 0 U PA2
4 0 U VSS
5 0 U PA8
6 0 U VDD
7 0 U PA3
8 0 U PA5
9 0 U PA4
10 0 U PA11
11 0 U PA13
12 0 U PA15
13 0 U PA6
14 0 U PA7
15 0 U PA9
16 0 U PA10
17 0 U PA12
18 0 U PA14
19 0 U PB0
20 0 U PB1
21 0 U GND



*PART*       ITEMS



C31          CAP0805          3902  7044    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-142 -174 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-182 -354 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" CAP0805
0 20 -80 0 0
1 20 -80 0 0

C7           CAP0805          1738  7122    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-108 -142 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-178 -332 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" CAP0805
0 20 -80 0 0
1 20 -80 0 0

J7           CONDIP2_A        5402  7244   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

D4           LED0805          4752  7144   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 -100 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

U2           AMS1117-3.3      3202  7344    0 0 97 10 97 10 4 1 4 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
190 52 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
200 -500 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
200 -600 0 6 97 10 0 "Regular Arial Unicode MS"
*
200 -700 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SOT223
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1

J3           CONDIP2_A        1254  7244   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R5           RES0402          4802  6544   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
34 -108 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
104 -108 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

J6           CONDIP2_A        5402  6894   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

C2           CAP0402          2138  7122    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C11          CAP0402          4252  7044    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-172 -154 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-222 -364 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

S7           SW_2P            10364 2756    0 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

S6           SW_2P            7948  3106   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R8           RES0402          9964  3206   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
66 -116 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
146 -126 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R9           RES0402          7998  2606   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
56 158 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
116 158 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

C37          CAP0402          9914  2656    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -210 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 -240 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

J9           CONDIP2_A        7548  2756   90 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

D1           LED0805          9200  6200   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D2           LED0805          9900  6200   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D3           LED0805          10600 5750   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

S1           SW_2P            7600  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R6           RES0402          7650  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 160 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
120 170 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

S2           SW_2P            8000  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R7           RES0402          8050  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
60 160 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
120 180 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

S3           SW_2P            8400  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R10          RES0402          8450  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
40 170 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
140 170 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R1           RES0402          9250  5500   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
40 -90 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
120 -100 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R2           RES0402          9950  5500   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
40 -110 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
120 -120 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R3           RES0402          10650 5640   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
60 -100 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
130 -100 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

J13          CONDIP2_A        7400  7100   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J14          CONDIP2_A        7400  6800   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J15          CONDIP2_A        7400  6500   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J16          CONDIP2_A        9200  6550    0 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-140 -10 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J17          CONDIP2_A        9900  6550    0 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-140 -10 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J18          CONDIP2_A        10600 6550    0 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-120 -10 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J11          CONDIP2_A        9610  2756   90 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J8           CONDIP2_A        2056  7448   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
154 8 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J1           HEAD2X16         1900  718     0 0 97 10 97 10 4 1 32 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
110 1742 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
120 -48 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
750 -40 0 6 97 10 0 "Regular Arial Unicode MS"
*
750 -140 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 2.54MM_CON2X16P
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1

R16          RES0402          1382  2168    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
280 -42 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
298 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R21          RES0402          2450  2168    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-90 -42 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-90 148 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R13          RES0402          1350  1268    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
290 -42 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
290 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R14          RES0402          2450  1268    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 -32 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-80 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

J2           HEAD2X16         4700  718     0 0 97 10 97 10 4 1 32 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 1742 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
100 -58 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
750 -40 0 6 97 10 0 "Regular Arial Unicode MS"
*
750 -140 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 2.54MM_CON2X16P
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1

R22          RES0402          4192  2168    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
298 -32 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
298 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R23          RES0402          5250  2168    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-100 -32 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-90 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R25          RES0402          4150  1068    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
280 -32 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
290 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

R26          RES0402          5250  1068    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 -32 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-90 138 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" RES0402
0 60 10 0 1
1 60 10 0 1

C50          CAP0603          2480  2878   90 2 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-32 -160 90 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-112 -540 90 1 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" CAP0603
0 20 -90 0 0
1 20 -80 0 0

C51          CAP0402          2480  3178   90 2 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-32 -160 90 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-122 -540 90 1 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

U1           N32A003F5Q7      2892  3416    0 0 97 10 97 10 4 1 21 0 0 0
"Default Font"
"Default Font"
588 654 0 0 97 10 0 "Default Font"
REF-DES
368 594 0 2 97 10 0 "Default Font"
PART-TYPE
1200 -140 0 2 97 10 0 "Default Font"
*
1200 -240 0 2 97 10 0 "Default Font"
*
"PCB DECAL" NS-QFN20-40P300X300X60-J150X150
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 1938   6322   0 0 0
@@@O1    GND $GND_SYMS 4752   6244   0 0 0
@@@O2    GND $GND_SYMS 4002   6244   0 0 0
@@@O3    GND $GND_SYMS 3002   6844   0 0 0
@@@O4    VDD_MCU $PWR_SYMS 5702   7244   90 1 0
@@@O5    5V $PWR_SYMS 970    7424   0 0 0
@@@O6    VDD_LINK $PWR_SYMS 5702   6894   90 1 0
@@@O7    GND $GND_SYMS 10814  2456   0 0 0
@@@O8    GND $GND_SYMS 9914   2156   0 0 0
@@@O9    VDD_MCU $PWR_SYMS 9914   3406   0 0 0
@@@O10   VDD_MCU $PWR_SYMS 7948   3456   0 0 0
@@@O11   GND $GND_SYMS 7948   2256   0 0 0
@@@O12   PA1 $OSR_SYMS 7248   2756   0 0 0
@@@O13   PA6 $OSR_SYMS 9200   6850   90 2 0
@@@O14   PA7 $OSR_SYMS 9900   6850   90 2 0
@@@O15   PA10 $OSR_SYMS 10600  6850   90 2 0
@@@O16   GND $GND_SYMS 9200   5150   0 0 0
@@@O17   GND $GND_SYMS 9900   5150   0 0 0
@@@O18   GND $GND_SYMS 7600   5200   0 0 0
@@@O19   GND $GND_SYMS 8000   5200   0 0 0
@@@O20   PA11 $OSR_SYMS 7150   6500   0 0 0
@@@O21   PA12 $OSR_SYMS 7150   6800   0 0 0
@@@O22   PA13 $OSR_SYMS 7150   7100   0 0 0
@@@O23   VDD_MCU $PWR_SYMS 10600  5300   0 2 0
@@@O24   VDD_MCU $PWR_SYMS 8400   5270   0 2 0
@@@O25   PA0 $OSR_SYMS 9346   2756   0 0 0
@@@O26   VDD_MCU $PWR_SYMS 2316   7448   90 1 0
@@@O27   VDD_MCU $PWR_SYMS 2600   2318   90 1 0
@@@O28   VDD_MCU $PWR_SYMS 1400   2318   90 0 0
@@@O29   VDD_MCU $PWR_SYMS 1400   2218   90 0 0
@@@O30   VDD_MCU $PWR_SYMS 2600   2218   90 1 0
@@@O31   VDD_MCU $PWR_SYMS 2850   2118   90 1 0
@@@O32   VDD_MCU $PWR_SYMS 1250   2118   90 0 0
@@@O33   PA0 $OSR_SYMS 1550   2018   0 0 0
@@@O34   PA0 $OSR_SYMS 2450   2018   0 1 0
@@@O35   PA1 $OSR_SYMS 1550   1918   0 0 0
@@@O36   PA1 $OSR_SYMS 2450   1918   0 1 0
@@@O37   PA2/TX1 $OSR_SYMS 1550   1818   0 0 0
@@@O38   PA2/TX1 $OSR_SYMS 2450   1818   0 1 0
@@@O39   PA8/SWDIO $OSR_SYMS 1550   1718   0 0 0
@@@O40   PA8/SWDIO $OSR_SYMS 2450   1718   0 1 0
@@@O41   PA3/RX1 $OSR_SYMS 1550   1618   0 0 0
@@@O42   PA5 $OSR_SYMS 1550   1518   0 0 0
@@@O43   PA4 $OSR_SYMS 1550   1418   0 0 0
@@@O44   PA11 $OSR_SYMS 1550   1318   0 0 0
@@@O45   PA3/RX1 $OSR_SYMS 2450   1618   0 1 0
@@@O46   PA5 $OSR_SYMS 2450   1518   0 1 0
@@@O47   PA4 $OSR_SYMS 2450   1418   0 1 0
@@@O48   PA11 $OSR_SYMS 2450   1318   0 1 0
@@@O49   GND $GND_SYMS 1200   1218   90 1 0
@@@O50   GND $GND_SYMS 3100   1218   90 0 0
@@@O51   GND $GND_SYMS 2500   1118   90 0 0
@@@O52   GND $GND_SYMS 2500   1018   90 0 0
@@@O53   GND $GND_SYMS 2500   918    90 0 0
@@@O54   GND $GND_SYMS 2500   818    90 0 0
@@@O55   GND $GND_SYMS 1550   1118   90 1 0
@@@O56   GND $GND_SYMS 1550   1018   90 1 0
@@@O57   GND $GND_SYMS 1550   918    90 1 0
@@@O58   GND $GND_SYMS 1550   818    90 1 0
@@@O59   VDD_MCU $PWR_SYMS 5400   2318   90 1 0
@@@O60   VDD_MCU $PWR_SYMS 4200   2318   90 0 0
@@@O61   VDD_MCU $PWR_SYMS 4200   2218   90 0 0
@@@O62   VDD_MCU $PWR_SYMS 5400   2218   90 1 0
@@@O63   VDD_MCU $PWR_SYMS 5650   2118   90 1 0
@@@O64   VDD_MCU $PWR_SYMS 4050   2118   90 0 0
@@@O65   PB1 $OSR_SYMS 4350   2018   0 0 0
@@@O66   PB1 $OSR_SYMS 5250   2018   0 1 0
@@@O67   PB0 $OSR_SYMS 4350   1918   0 0 0
@@@O68   PB0 $OSR_SYMS 5250   1918   0 1 0
@@@O69   PA14 $OSR_SYMS 4350   1818   0 0 0
@@@O70   PA14 $OSR_SYMS 5250   1818   0 1 0
@@@O71   PA12 $OSR_SYMS 4350   1718   0 0 0
@@@O72   PA12 $OSR_SYMS 5250   1718   0 1 0
@@@O73   PA10 $OSR_SYMS 4350   1618   0 0 0
@@@O74   PA9/SWDCK $OSR_SYMS 4350   1518   0 0 0
@@@O75   PA7 $OSR_SYMS 4350   1418   0 0 0
@@@O76   PA6 $OSR_SYMS 4350   1318   0 0 0
@@@O77   PA10 $OSR_SYMS 5250   1618   0 1 0
@@@O78   PA9/SWDCK $OSR_SYMS 5250   1518   0 1 0
@@@O79   PA7 $OSR_SYMS 5250   1418   0 1 0
@@@O80   PA6 $OSR_SYMS 5250   1318   0 1 0
@@@O81   GND $GND_SYMS 4000   1018   90 1 0
@@@O82   GND $GND_SYMS 5800   1018   90 0 0
@@@O83   GND $GND_SYMS 5300   918    90 0 0
@@@O84   GND $GND_SYMS 5300   818    90 0 0
@@@O85   GND $GND_SYMS 4350   918    90 1 0
@@@O86   GND $GND_SYMS 4350   818    90 1 0
@@@O87   PA15 $OSR_SYMS 4350   1218   0 0 0
@@@O88   PA13 $OSR_SYMS 4350   1118   0 0 0
@@@O89   PA15 $OSR_SYMS 5250   1218   0 1 0
@@@O90   PA13 $OSR_SYMS 5250   1118   0 1 0
@@@O91   PA0 $OSR_SYMS 2492   4216   0 0 0
@@@O92   PA2/TX1 $OSR_SYMS 2492   4016   0 0 0
@@@O93   PA1 $OSR_SYMS 2492   4116   0 0 0
@@@O94   PA8/SWDIO $OSR_SYMS 2492   3816   0 0 0
@@@O95   PA3/RX1 $OSR_SYMS 3392   3116   90 0 0
@@@O96   PA5 $OSR_SYMS 3492   3116   90 0 0
@@@O97   PA4 $OSR_SYMS 3592   3116   90 0 0
@@@O98   PA11 $OSR_SYMS 3692   3116   90 0 0
@@@O99   PA9/SWDCK $OSR_SYMS 4492   4216   0 1 0
@@@O100  PA7 $OSR_SYMS 4492   4116   0 1 0
@@@O101  PA13 $OSR_SYMS 4492   3816   0 1 0
@@@O102  PA10 $OSR_SYMS 3692   4866   90 2 0
@@@O103  PA12 $OSR_SYMS 3592   4866   90 3 0
@@@O104  PB1 $OSR_SYMS 3292   4866   90 2 0
@@@O105  GND $GND_SYMS 2342   2816   0 1 0
@@@O106  PA14 $OSR_SYMS 3492   4866   90 2 0
@@@O107  PB0 $OSR_SYMS 3392   4866   90 2 0
@@@O108  GND $GND_SYMS 2592   3916   90 1 0
@@@O109  VDD_MCU $PWR_SYMS 3292   3020   0 2 0
@@@O110  PA15 $OSR_SYMS 4492   3916   0 1 0
@@@O111  PA6 $OSR_SYMS 4492   4016   0 3 0
@@@O112  GND $GND_SYMS 3192   4874   0 2 0

*TIEDOTS*



@@@D0    3902   7244  
@@@D1    4752   7244  
@@@D2    5102   7244  
@@@D3    1938   6472  
@@@D4    4002   6444  
@@@D5    4252   7244  
@@@D6    9914   2756  
@@@D7    7948   2756  
@@@D8    3802   7244  
@@@D9    9914   2756  
@@@D10   1738   7244  
@@@D11   2138   7244  
@@@D12   1738   7244  
@@@D13   2342   2878  
@@@D14   3292   3178  
@@@D15   3092   3178  

*CONNECTION*


*SIGNAL* $$$6153 64 0
S7.1         @@@D9        2 0
10164  2756  
9914   2756  
C37.1        @@@D6        2 0
9914   2656  
9914   2756  
R8.2         @@@D6        2 0
9914   2906  
9914   2756  
J11.2        @@@D9        2 0
9810   2756  
9914   2756  
@@@D9        @@@D6        2 0
9914   2756  
9914   2756  

*SIGNAL* PA1 0 0
J9.1         @@@O12       2 0
7348   2756  
7248   2756  
J1.9         @@@O35       2 0
1700   1918  
1550   1918  
J1.10        @@@O36       2 0
2300   1918  
2450   1918  
U1.2         @@@O93       2 0
2692   4116  
2492   4116  

*SIGNAL* PA4 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J1.19        @@@O43       2 0
1700   1418  
1550   1418  
J1.20        @@@O47       2 0
2300   1418  
2450   1418  
U1.9         @@@O97       2 0
3592   3216  
3592   3116  

*SIGNAL* PA5 0 0
J1.17        @@@O42       2 0
1700   1518  
1550   1518  
J1.18        @@@O46       2 0
2300   1518  
2450   1518  
U1.8         @@@O96       2 0
3492   3216  
3492   3116  

*SIGNAL* PA6 0 0
J16.1        @@@O13       2 0
9200   6750  
9200   6850  
J2.21        @@@O76       2 0
4500   1318  
4350   1318  
J2.22        @@@O80       2 0
5100   1318  
5250   1318  
U1.13        @@@O111      2 0
4292   4016  
4492   4016  

*SIGNAL* PA7 0 0
J17.1        @@@O14       2 0
9900   6750  
9900   6850  
J2.19        @@@O75       2 0
4500   1418  
4350   1418  
J2.20        @@@O79       2 0
5100   1418  
5250   1418  
U1.14        @@@O100      2 0
4292   4116  
4492   4116  

*SIGNAL* $$$14234 64 0
R21.1        J1.6         2 0
2350   2118  
2300   2118  

*SIGNAL* PA8/SWDIO 0 0
J1.13        @@@O39       2 0
1700   1718  
1550   1718  
J1.14        @@@O40       2 0
2300   1718  
2450   1718  
U1.5         @@@O94       2 0
2692   3816  
2492   3816  

*SIGNAL* PA2/TX1 0 0
J1.11        @@@O37       2 0
1700   1818  
1550   1818  
J1.12        @@@O38       2 0
2300   1818  
2450   1818  
U1.3         @@@O92       2 0
2692   4016  
2492   4016  

*SIGNAL* PA9/SWDCK 0 0
J2.17        @@@O74       2 0
4500   1518  
4350   1518  
J2.18        @@@O78       2 0
5100   1518  
5250   1518  
U1.15        @@@O99       2 0
4292   4216  
4492   4216  

*SIGNAL* PA14 0 0
J2.11        @@@O69       2 0
4500   1818  
4350   1818  
J2.12        @@@O70       2 0
5100   1818  
5250   1818  
U1.18        @@@O106      2 0
3492   4816  
3492   4866  

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
@@@O4        J7.1         2 0
5702   7244  
5602   7244  
R8.1         @@@O9        2 0
9914   3306  
9914   3406  
@@@O10       S6.2         2 0
7948   3456  
7948   3306  
R3.2         @@@O23       2 0
10600  5340  
10600  5300  
R10.2        @@@O24       2 0
8400   5350  
8400   5270  
J8.1         @@@O26       2 0
2256   7448  
2316   7448  
J1.2         @@@O27       2 0
2300   2318  
2600   2318  
J1.1         @@@O28       2 0
1700   2318  
1400   2318  
J1.3         @@@O29       2 0
1700   2218  
1400   2218  
J1.4         @@@O30       2 0
2300   2218  
2600   2218  
R21.2        @@@O31       2 0
2750   2118  
2850   2118  
R16.1        @@@O32       2 0
1282   2118  
1250   2118  
J2.2         @@@O59       2 0
5100   2318  
5400   2318  
J2.1         @@@O60       2 0
4500   2318  
4200   2318  
J2.3         @@@O61       2 0
4500   2218  
4200   2218  
J2.4         @@@O62       2 0
5100   2218  
5400   2218  
R23.2        @@@O63       2 0
5550   2118  
5650   2118  
R22.1        @@@O64       2 0
4092   2118  
4050   2118  
U1.6         @@@D14       2 0
3292   3216  
3292   3178  
C51.2        @@@D15       2 0
2980   3178  
3092   3178  
@@@D14       @@@O109      2 0
3292   3178  
3292   3020  
@@@D15       @@@D14       2 0
3092   3178  
3292   3178  
@@@D15       C50.2        3 0
3092   3178  
3092   2878  
2980   2878  

*SIGNAL* PB1 0 0
J2.7         @@@O65       2 0
4500   2018  
4350   2018  
J2.8         @@@O66       2 0
5100   2018  
5250   2018  
U1.20        @@@O104      2 0
3292   4816  
3292   4866  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        @@@D3        2 0
1938   6322  
1938   6472  
@@@O1        R5.2         2 0
4752   6244  
4752   6244  
C31.2        @@@D4        3 0
3902   6544  
3902   6444  
4002   6444  
U2.1         @@@O3        2 0
3002   7044  
3002   6844  
@@@D3        C7.2         3 0
1938   6472  
1738   6472  
1738   6622  
@@@D3        C2.2         3 0
1938   6472  
2138   6472  
2138   6622  
@@@D4        @@@O2        2 0
4002   6444  
4002   6244  
@@@D4        C11.2        3 0
4002   6444  
4252   6444  
4252   6544  
@@@O7        S7.2         3 0
10814  2456  
10814  2756  
10564  2756  
C37.2        @@@O8        2 0
9914   2156  
9914   2156  
R9.2         @@@O11       2 0
7948   2306  
7948   2256  
R1.2         @@@O16       2 0
9200   5200  
9200   5150  
R2.2         @@@O17       2 0
9900   5200  
9900   5150  
R6.2         @@@O18       2 0
7600   5350  
7600   5200  
R7.2         @@@O19       2 0
8000   5350  
8000   5200  
R13.1        @@@O49       2 0
1250   1218  
1200   1218  
R14.2        @@@O50       2 0
2750   1218  
3100   1218  
J1.26        @@@O51       2 0
2300   1118  
2500   1118  
J1.28        @@@O52       2 0
2300   1018  
2500   1018  
J1.30        @@@O53       2 0
2300   918   
2500   918   
J1.32        @@@O54       2 0
2300   818   
2500   818   
J1.25        @@@O55       2 0
1700   1118  
1550   1118  
J1.27        @@@O56       2 0
1700   1018  
1550   1018  
J1.29        @@@O57       2 0
1700   918   
1550   918   
J1.31        @@@O58       2 0
1700   818   
1550   818   
R25.1        @@@O81       2 0
4050   1018  
4000   1018  
R26.2        @@@O82       2 0
5550   1018  
5800   1018  
J2.30        @@@O83       2 0
5100   918   
5300   918   
J2.32        @@@O84       2 0
5100   818   
5300   818   
J2.29        @@@O85       2 0
4500   918   
4350   918   
J2.31        @@@O86       2 0
4500   818   
4350   818   
C51.1        @@@D13       3 0
2480   3178  
2342   3178  
2342   2878  
C50.1        @@@D13       2 0
2480   2878  
2342   2878  
U1.4         @@@O108      2 0
2692   3916  
2592   3916  
@@@D13       @@@O105      2 0
2342   2878  
2342   2816  
U1.21        @@@O112      2 0
3192   4816  
3192   4874  

*SIGNAL* PB0 0 0
J2.9         @@@O67       2 0
4500   1918  
4350   1918  
J2.10        @@@O68       2 0
5100   1918  
5250   1918  
U1.19        @@@O107      2 0
3392   4816  
3392   4866  

*SIGNAL* $$$14321 64 0
J1.5         R16.2        2 0
1700   2118  
1682   2118  

*SIGNAL* PA12 0 0
J14.2        @@@O21       2 0
7200   6800  
7150   6800  
J2.13        @@@O71       2 0
4500   1718  
4350   1718  
J2.14        @@@O72       2 0
5100   1718  
5250   1718  
U1.17        @@@O103      2 0
3592   4816  
3592   4866  

*SIGNAL* $$$27316 64 0
J1.23        R13.2        2 0
1700   1218  
1650   1218  

*SIGNAL* PA0 0 0
J11.1        @@@O25       2 0
9410   2756  
9346   2756  
J1.7         @@@O33       2 0
1700   2018  
1550   2018  
J1.8         @@@O34       2 0
2300   2018  
2450   2018  
U1.1         @@@O91       2 0
2692   4216  
2492   4216  

*SIGNAL* PA10 0 0
J18.1        @@@O15       2 0
10600  6750  
10600  6850  
J2.15        @@@O73       2 0
4500   1618  
4350   1618  
J2.16        @@@O77       2 0
5100   1618  
5250   1618  
U1.16        @@@O102      2 0
3692   4816  
3692   4866  

*SIGNAL* $$$27329 64 0
R14.1        J1.24        2 0
2350   1218  
2300   1218  

*SIGNAL* $$$16580 64 0
J3.1         @@@D10       2 0
1454   7244  
1738   7244  
C7.1         @@@D12       2 0
1738   7122  
1738   7244  
@@@D10       @@@D11       2 0
1738   7244  
2138   7244  
C2.1         @@@D11       3 0
2138   7122  
2138   7244  
2138   7244  
@@@D11       U2.3         2 0
2138   7244  
3002   7244  
@@@D12       @@@D10       2 0
1738   7244  
1738   7244  
@@@D12       J8.2         3 0
1738   7244  
1738   7448  
1856   7448  

*SIGNAL* $$$18572 64 0
@@@D0        @@@D5        2 0
3902   7244  
4252   7244  
@@@D0        @@@D8        2 0
3902   7244  
3802   7244  
C31.1        @@@D0        2 0
3902   7044  
3902   7244  
D4.2         @@@D1        2 0
4752   7144  
4752   7244  
@@@D1        @@@D2        2 0
4752   7244  
5102   7244  
J6.2         @@@D2        3 0
5202   6894  
5102   6894  
5102   7244  
@@@D2        J7.2         2 0
5102   7244  
5202   7244  
C11.1        @@@D5        2 0
4252   7044  
4252   7244  
@@@D5        @@@D1        2 0
4252   7244  
4752   7244  
U2.2         @@@D8        2 0
3802   7044  
3802   7244  
@@@D8        U2.4         2 0
3802   7244  
3802   7244  

*SIGNAL* 5V 0 0
@@@O5        J3.2         3 0
970    7424  
970    7244  
1054   7244  

*SIGNAL* $$$23084 64 0
R5.1         D4.1         2 0
4752   6644  
4752   6644  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J6.1         @@@O6        2 0
5602   6894  
5702   6894  

*SIGNAL* $$$13829 64 0
S6.1         @@@D7        2 0
7948   2906  
7948   2756  
R9.1         @@@D7        2 0
7948   2706  
7948   2756  
@@@D7        J9.2         2 0
7948   2756  
7748   2756  

*SIGNAL* $$$2339 64 0
R1.1         D1.1         2 0
9200   5600  
9200   5700  

*SIGNAL* $$$2340 64 0
R2.1         D2.1         2 0
9900   5600  
9900   5700  

*SIGNAL* $$$28366 64 0
R23.1        J2.6         2 0
5150   2118  
5100   2118  

*SIGNAL* $$$7234 64 0
D1.2         J16.2        2 0
9200   6200  
9200   6350  

*SIGNAL* $$$28367 64 0
J2.5         R22.2        2 0
4500   2118  
4492   2118  

*SIGNAL* $$$13605 64 0
R6.1         S1.1         2 0
7600   5750  
7600   5850  

*SIGNAL* $$$13607 64 0
S2.1         R7.1         2 0
8000   5850  
8000   5750  

*SIGNAL* $$$13609 64 0
S3.1         R10.1        2 0
8400   5850  
8400   5750  

*SIGNAL* $$$6888 64 0
S1.2         J15.1        2 0
7600   6250  
7600   6500  

*SIGNAL* $$$6886 64 0
S2.2         J14.1        3 0
8000   6250  
8000   6800  
7600   6800  

*SIGNAL* $$$6884 64 0
S3.2         J13.1        3 0
8400   6250  
8400   7100  
7600   7100  

*SIGNAL* $$$7236 64 0
D2.2         J17.2        2 0
9900   6200  
9900   6350  

*SIGNAL* $$$29131 64 0
R26.1        J2.28        2 0
5150   1018  
5100   1018  

*SIGNAL* $$$29134 64 0
J2.27        R25.2        2 0
4500   1018  
4450   1018  

*SIGNAL* PA3/RX1 0 0
J1.15        @@@O41       2 0
1700   1618  
1550   1618  
J1.16        @@@O45       2 0
2300   1618  
2450   1618  
U1.7         @@@O95       2 0
3392   3216  
3392   3116  

*SIGNAL* $$$1150 64 0
D3.1         J18.2        2 0
10600  6250  
10600  6350  

*SIGNAL* PA15 0 0
J2.23        @@@O87       2 0
4500   1218  
4350   1218  
J2.24        @@@O89       2 0
5100   1218  
5250   1218  
U1.12        @@@O110      2 0
4292   3916  
4492   3916  

*SIGNAL* PA13 0 0
J13.2        @@@O22       2 0
7200   7100  
7150   7100  
J2.25        @@@O88       2 0
4500   1118  
4350   1118  
J2.26        @@@O90       2 0
5100   1118  
5250   1118  
U1.11        @@@O101      2 0
4292   3816  
4492   3816  

*SIGNAL* PA11 0 0
J15.2        @@@O20       2 0
7200   6500  
7150   6500  
J1.21        @@@O44       2 0
1700   1318  
1550   1318  
J1.22        @@@O48       2 0
2300   1318  
2450   1318  
U1.10        @@@O98       2 0
3692   3216  
3692   3116  

*SIGNAL* $$$1153 64 0
R3.1         D3.2         2 0
10600  5740  
10600  5750  

*NETNAMES*



VDD_MCU      @@@O4        400    50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
5V           @@@O5        -2     226    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O6        400    50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O9        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O10       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O12       -338   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA6          @@@O13       0      360    90 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA7          @@@O14       0      360    90 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA10         @@@O15       50     500    90 2 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA11         @@@O20       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O21       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13         @@@O22       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O23       10     -350   0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O24       -38    -332   0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O25       -362   -32    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O26       432    -34    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O27       438    -20    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O28       -400   50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O31       412    -26    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O30       430    -16    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O29       -410   -38    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O32       -388   -44    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O33       -400   -40    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O34       376    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O35       -390   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O36       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2/TX1      @@@O37       -390   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2/TX1      @@@O38       370    -40    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA8/SWDIO    @@@O39       -390   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA8/SWDIO    @@@O40       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3/RX1      @@@O41       -390   -20    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA5          @@@O42       -400   -20    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA4          @@@O43       -400   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA11         @@@O44       -400   -40    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3/RX1      @@@O45       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA5          @@@O46       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA4          @@@O47       370    -40    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA11         @@@O48       370    -50    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O59       438    -20    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O60       -400   50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O63       412    -26    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O62       430    -16    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O61       -410   -38    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O64       -388   -44    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PB1          @@@O65       -400   -40    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB1          @@@O66       370    -20    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O67       -400   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O68       370    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14         @@@O69       -360   -38    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14         @@@O70       370    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O71       -360   -38    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O72       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA10         @@@O73       -360   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA9/SWDCK    @@@O74       -350   -38    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA7          @@@O75       -400   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA6          @@@O76       -400   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA10         @@@O77       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA9/SWDCK    @@@O78       370    -30    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA7          @@@O79       370    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA6          @@@O80       370    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA15         @@@O87       -360   -38    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13         @@@O88       -360   -38    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA15         @@@O89       370    -38    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13         @@@O90       370    -40    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O91       -362   -28    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2/TX1      @@@O92       -352   -18    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O93       -352   -28    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA8/SWDIO    @@@O94       -356   -34    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3/RX1      @@@O95       28     -344   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA5          @@@O96       34     -346   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA4          @@@O97       36     -346   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA11         @@@O98       42     -320   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA9/SWDCK    @@@O99       364    -32    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA7          @@@O100      364    -26    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13         @@@O101      370    -38    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA10         @@@O102      -28    522    90 3 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O103      -36    352    90 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB1          @@@O104      -30    484    90 3 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14         @@@O106      -38    522    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O107      -28    484    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O109      20     -414   90 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA15         @@@O110      368    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA6          @@@O111      368    -28    0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"

*END*     OF ASCII OUTPUT FILE