*PADS-LOGIC-V9.0-CP936* DESIGN EXPORT FILE FROM PADS LOGIC VVX.2.7
*SCH*        GENERAL PARAMETERS OF THE SCHEMATIC DESIGN"

CUR SHEET    1              Current Active Sheet
USERGRID     50     2       Design and Label/Text grid settings
LINEWIDTH    10             Width items will be created with
CONNWIDTH    10             Width used to plot connections
BUSWIDTH     25             Width used to plot buses
BUSANGLE     25             Angle used when plotting buses
NNVISPWRGND  4              Pwr/Gnd netname visibility default flag
PCBFLAGS     1039           PCB Netlist and ECO options
PINNAMESIZE  97     10      Height and LineWidth used by pin names
TEXTSIZE     97     10      Height and LineWidth text will be created width
JOBTIME      0              Amount of time spent on this LOGIC design
DOTGRID      100            Space in thous/inch between graphic dots
BACKUPTIME   5              Number of minutes between database backups
TIEDOTSIZE   75             Diameter of tiedot point
REFNAMESIZE  100    10      Height and LineWidth used by part ref. names
PARTNAMESIZE 100    10      Height and LineWidth used by part type names
PINNOSIZE    97     10      Height and LineWidth used by pin numbers
NETNAMESIZE  100    10      Height and LineWidth used by net names
REAL WIDTH   36             Widths greater then this are displayed real size
SHEET SIZE   A4            
UNITS        0              Rules units type
JOBNAME      N32A052KBQX_STB_V1.0.sch
NTXCOL 11 9
HIRCOL 14
LINCOL 4
TXTCOL 0 15
CONCOL 4
BUSCOL 14
PTXCOL 0 15
COMCOL 9
NMCOL  12 15
PNMCOL 12 15
PINCOL 0 15
NETCOL 9 15
FBGCOL 12 15
OFFREFVIEW   0              Offsheet references visibility default flag
OFFREFNUM    0              Offsheet references per line
SHEETNUMSEP  []             Sheet Number separators
FONT MODE   System
DEFAULT FONT "Regular Tahoma"
BORDER NAME DRW_NATIONS_A4
FIELDCOL 9 15

*CAM* PLOTTER SETTINGS 
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

PLOT_SECTION	5.0
{
PLOT_DEFAULTS_PHOTO_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_MPOS_V1
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Current
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PEN_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_FNT_V0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 Y
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Selected
DEFAULT_SHEET_LIST	NULL
{
SHEET_1	2
SHEET_2	4
SHEET_3	5
SHEET_4	6
SHEET_5	8
SHEET_6	1
SHEET_7	7
}
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PRINTER	NULL
{
DEFAULT_FILE_PREFIX	 NZ3101_FNT_BCM_0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	All
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_AUGMENT_ON_THE_FLY	Y
}

*MISC*      MISCELLANEOUS PARAMETERS
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	MILS
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	Top
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ASSOCIATED_SILK_SCREEN	Silkscreen Top
ASSOCIATED_PASTE_MASK	Paste Mask Top
ASSOCIATED_SOLDER_MASK	Solder Mask Top
ASSOCIATED_ASSEMBLY	Assembly Drawing Top
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	Bottom
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Layer_3
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	4
{
LAYER_NAME	Layer_4
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	Layer_21
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Layer_22
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Layer_23
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	Layer_24
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Layer_26
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	Layer_27
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	Layer_28
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Layer_29
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	Layer_30
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	31
{
LAYER_NAME	Layer_31
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	32
{
LAYER_NAME	Layer_32
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	33
{
LAYER_NAME	Layer_33
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	34
{
LAYER_NAME	Layer_34
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	35
{
LAYER_NAME	Layer_35
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	36
{
LAYER_NAME	Layer_36
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	37
{
LAYER_NAME	Layer_37
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	38
{
LAYER_NAME	Layer_38
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	39
{
LAYER_NAME	Layer_39
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	40
{
LAYER_NAME	Layer_40
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	41
{
LAYER_NAME	Layer_41
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	42
{
LAYER_NAME	Layer_42
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	43
{
LAYER_NAME	Layer_43
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	44
{
LAYER_NAME	Layer_44
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	45
{
LAYER_NAME	Layer_45
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	46
{
LAYER_NAME	Layer_46
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	47
{
LAYER_NAME	Layer_47
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	48
{
LAYER_NAME	Layer_48
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	49
{
LAYER_NAME	Layer_49
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	50
{
LAYER_NAME	Layer_50
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	51
{
LAYER_NAME	Layer_51
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	52
{
LAYER_NAME	Layer_52
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	53
{
LAYER_NAME	Layer_53
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	54
{
LAYER_NAME	Layer_54
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	55
{
LAYER_NAME	Layer_55
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	56
{
LAYER_NAME	Layer_56
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	57
{
LAYER_NAME	Layer_57
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	58
{
LAYER_NAME	Layer_58
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	59
{
LAYER_NAME	Layer_59
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	60
{
LAYER_NAME	Layer_60
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	61
{
LAYER_NAME	Layer_61
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	62
{
LAYER_NAME	Layer_62
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	63
{
LAYER_NAME	Layer_63
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	64
{
LAYER_NAME	Layer_64
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	65
{
LAYER_NAME	Layer_65
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	66
{
LAYER_NAME	Layer_66
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	67
{
LAYER_NAME	Layer_67
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	68
{
LAYER_NAME	Layer_68
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	69
{
LAYER_NAME	Layer_69
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	70
{
LAYER_NAME	Layer_70
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	71
{
LAYER_NAME	Layer_71
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	72
{
LAYER_NAME	Layer_72
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	73
{
LAYER_NAME	Layer_73
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	74
{
LAYER_NAME	Layer_74
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	75
{
LAYER_NAME	Layer_75
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	76
{
LAYER_NAME	Layer_76
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	77
{
LAYER_NAME	Layer_77
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	78
{
LAYER_NAME	Layer_78
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	79
{
LAYER_NAME	Layer_79
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	80
{
LAYER_NAME	Layer_80
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	81
{
LAYER_NAME	Layer_81
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	82
{
LAYER_NAME	Layer_82
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	83
{
LAYER_NAME	Layer_83
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	84
{
LAYER_NAME	Layer_84
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	85
{
LAYER_NAME	Layer_85
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	86
{
LAYER_NAME	Layer_86
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	87
{
LAYER_NAME	Layer_87
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	88
{
LAYER_NAME	Layer_88
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	89
{
LAYER_NAME	Layer_89
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	90
{
LAYER_NAME	Layer_90
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	91
{
LAYER_NAME	Layer_91
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	92
{
LAYER_NAME	Layer_92
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	93
{
LAYER_NAME	Layer_93
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	94
{
LAYER_NAME	Layer_94
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	95
{
LAYER_NAME	Layer_95
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	96
{
LAYER_NAME	Layer_96
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	97
{
LAYER_NAME	Layer_97
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	98
{
LAYER_NAME	Layer_98
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	99
{
LAYER_NAME	Layer_99
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	100
{
LAYER_NAME	Layer_100
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	101
{
LAYER_NAME	Layer_101
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	102
{
LAYER_NAME	Layer_102
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	103
{
LAYER_NAME	Layer_103
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	104
{
LAYER_NAME	Layer_104
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	105
{
LAYER_NAME	Layer_105
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	106
{
LAYER_NAME	Layer_106
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	107
{
LAYER_NAME	Layer_107
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	108
{
LAYER_NAME	Layer_108
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	109
{
LAYER_NAME	Layer_109
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	110
{
LAYER_NAME	Layer_110
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	111
{
LAYER_NAME	Layer_111
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	112
{
LAYER_NAME	Layer_112
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	113
{
LAYER_NAME	Layer_113
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	114
{
LAYER_NAME	Layer_114
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	115
{
LAYER_NAME	Layer_115
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	116
{
LAYER_NAME	Layer_116
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	117
{
LAYER_NAME	Layer_117
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	118
{
LAYER_NAME	Layer_118
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	119
{
LAYER_NAME	Layer_119
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	120
{
LAYER_NAME	Layer_120
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	121
{
LAYER_NAME	Solder Mask Top
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	122
{
LAYER_NAME	Paste Mask Bottom
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	123
{
LAYER_NAME	Paste Mask Top
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	124
{
LAYER_NAME	Drill Drawing
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	125
{
LAYER_NAME	Layer_125
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	126
{
LAYER_NAME	Silkscreen Top
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	127
{
LAYER_NAME	Assembly Drawing Top
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	128
{
LAYER_NAME	Solder Mask Bottom
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	129
{
LAYER_NAME	Silkscreen Bottom
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	130
{
LAYER_NAME	Assembly Drawing Bottom
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	131
{
LAYER_NAME	Layer_131
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	132
{
LAYER_NAME	Layer_132
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	133
{
LAYER_NAME	Layer_133
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	134
{
LAYER_NAME	Layer_134
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	135
{
LAYER_NAME	Layer_135
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	136
{
LAYER_NAME	Layer_136
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	137
{
LAYER_NAME	Layer_137
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	138
{
LAYER_NAME	Layer_138
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	139
{
LAYER_NAME	Layer_139
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	140
{
LAYER_NAME	Layer_140
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	141
{
LAYER_NAME	Layer_141
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	142
{
LAYER_NAME	Layer_142
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	143
{
LAYER_NAME	Layer_143
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	144
{
LAYER_NAME	Layer_144
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	145
{
LAYER_NAME	Layer_145
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	146
{
LAYER_NAME	Layer_146
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	147
{
LAYER_NAME	Layer_147
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	148
{
LAYER_NAME	Layer_148
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	149
{
LAYER_NAME	Layer_149
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	150
{
LAYER_NAME	Layer_150
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	151
{
LAYER_NAME	Layer_151
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	152
{
LAYER_NAME	Layer_152
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	153
{
LAYER_NAME	Layer_153
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	154
{
LAYER_NAME	Layer_154
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	155
{
LAYER_NAME	Layer_155
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	156
{
LAYER_NAME	Layer_156
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	157
{
LAYER_NAME	Layer_157
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	158
{
LAYER_NAME	Layer_158
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	159
{
LAYER_NAME	Layer_159
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	160
{
LAYER_NAME	Layer_160
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	161
{
LAYER_NAME	Layer_161
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	162
{
LAYER_NAME	Layer_162
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	163
{
LAYER_NAME	Layer_163
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	164
{
LAYER_NAME	Layer_164
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	165
{
LAYER_NAME	Layer_165
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	166
{
LAYER_NAME	Layer_166
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	167
{
LAYER_NAME	Layer_167
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	168
{
LAYER_NAME	Layer_168
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	169
{
LAYER_NAME	Layer_169
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	170
{
LAYER_NAME	Layer_170
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	171
{
LAYER_NAME	Layer_171
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	172
{
LAYER_NAME	Layer_172
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	173
{
LAYER_NAME	Layer_173
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	174
{
LAYER_NAME	Layer_174
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	175
{
LAYER_NAME	Layer_175
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	176
{
LAYER_NAME	Layer_176
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	177
{
LAYER_NAME	Layer_177
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	178
{
LAYER_NAME	Layer_178
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	179
{
LAYER_NAME	Layer_179
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	180
{
LAYER_NAME	Layer_180
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	181
{
LAYER_NAME	Layer_181
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	182
{
LAYER_NAME	Layer_182
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	183
{
LAYER_NAME	Layer_183
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	184
{
LAYER_NAME	Layer_184
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	185
{
LAYER_NAME	Layer_185
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	186
{
LAYER_NAME	Layer_186
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	187
{
LAYER_NAME	Layer_187
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	188
{
LAYER_NAME	Layer_188
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	189
{
LAYER_NAME	Layer_189
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	190
{
LAYER_NAME	Layer_190
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	191
{
LAYER_NAME	Layer_191
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	192
{
LAYER_NAME	Layer_192
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	193
{
LAYER_NAME	Layer_193
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	194
{
LAYER_NAME	Layer_194
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	195
{
LAYER_NAME	Layer_195
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	196
{
LAYER_NAME	Layer_196
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	197
{
LAYER_NAME	Layer_197
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	198
{
LAYER_NAME	Layer_198
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	199
{
LAYER_NAME	Layer_199
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	200
{
LAYER_NAME	Layer_200
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	201
{
LAYER_NAME	Layer_201
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	202
{
LAYER_NAME	Layer_202
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	203
{
LAYER_NAME	Layer_203
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	204
{
LAYER_NAME	Layer_204
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	205
{
LAYER_NAME	Layer_205
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	206
{
LAYER_NAME	Layer_206
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	207
{
LAYER_NAME	Layer_207
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	208
{
LAYER_NAME	Layer_208
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	209
{
LAYER_NAME	Layer_209
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	210
{
LAYER_NAME	Layer_210
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	211
{
LAYER_NAME	Layer_211
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	212
{
LAYER_NAME	Layer_212
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	213
{
LAYER_NAME	Layer_213
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	214
{
LAYER_NAME	Layer_214
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	215
{
LAYER_NAME	Layer_215
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	216
{
LAYER_NAME	Layer_216
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	217
{
LAYER_NAME	Layer_217
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	218
{
LAYER_NAME	Layer_218
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	219
{
LAYER_NAME	Layer_219
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	220
{
LAYER_NAME	Layer_220
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	221
{
LAYER_NAME	Layer_221
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	222
{
LAYER_NAME	Layer_222
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	223
{
LAYER_NAME	Layer_223
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	224
{
LAYER_NAME	Layer_224
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	225
{
LAYER_NAME	Layer_225
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	226
{
LAYER_NAME	Layer_226
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	227
{
LAYER_NAME	Layer_227
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	228
{
LAYER_NAME	Layer_228
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	229
{
LAYER_NAME	Layer_229
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	230
{
LAYER_NAME	Layer_230
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	231
{
LAYER_NAME	Layer_231
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	232
{
LAYER_NAME	Layer_232
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	233
{
LAYER_NAME	Layer_233
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	234
{
LAYER_NAME	Layer_234
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	235
{
LAYER_NAME	Layer_235
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	236
{
LAYER_NAME	Layer_236
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	237
{
LAYER_NAME	Layer_237
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	238
{
LAYER_NAME	Layer_238
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	239
{
LAYER_NAME	Layer_239
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	240
{
LAYER_NAME	Layer_240
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	241
{
LAYER_NAME	Layer_241
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	242
{
LAYER_NAME	Layer_242
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	243
{
LAYER_NAME	Layer_243
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	244
{
LAYER_NAME	Layer_244
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	245
{
LAYER_NAME	Layer_245
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	246
{
LAYER_NAME	Layer_246
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	247
{
LAYER_NAME	Layer_247
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	248
{
LAYER_NAME	Layer_248
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	249
{
LAYER_NAME	Layer_249
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	250
{
LAYER_NAME	Layer_250
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	MILS
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	10
COPPER_TO_VIA	10
COPPER_TO_PAD	10
COPPER_TO_SMD	10
COPPER_TO_COPPER	10
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	13
OUTLINE_TO_VIA	13
OUTLINE_TO_PAD	13
OUTLINE_TO_SMD	13
OUTLINE_TO_COPPER	13
DRILL_TO_TRACK	7
DRILL_TO_VIA	7
DRILL_TO_PAD	7
DRILL_TO_SMD	7
DRILL_TO_COPPER	7
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	50
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	50000
STUB_LENGTH	0
PARALLEL_LENGTH	1000
PARALLEL_GAP	200
TANDEM_LENGTH	1000
TANDEM_GAP	200
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	200
MATCH_LENGTH_TOLERANCE	200
}
}
RULE_SET	(4)
{
FOR	:
{
NET	PD15_OSC_OUT
NET	$$$29264
NET	$$$18547
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	20
COPPER_TO_VIA	20
COPPER_TO_PAD	20
COPPER_TO_SMD	20
COPPER_TO_COPPER	20
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	20
OUTLINE_TO_VIA	20
OUTLINE_TO_PAD	20
OUTLINE_TO_SMD	20
OUTLINE_TO_COPPER	20
DRILL_TO_TRACK	7
DRILL_TO_VIA	7
DRILL_TO_PAD	7
DRILL_TO_SMD	7
DRILL_TO_COPPER	7
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	30
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
DIF_PAIR	D1
{
NET	$$$24997
NET	$$$24935
MIN_LENGTH	0
MAX_LENGTH	448000
GAP	6
MAX_OBSTACLE_SIZE	25
MAX_OBSTACLE_NUMBER	3
WIDTH	6
LAYER_NAME	<Outer Layers>
{
WIDTH	6
GAP	6
}
}
DIF_PAIR	D2
{
NET	DM_NSLINK
NET	DP_NSLINK
MIN_LENGTH	0
MAX_LENGTH	448000
GAP	6
MAX_OBSTACLE_SIZE	25
MAX_OBSTACLE_NUMBER	3
WIDTH	6
LAYER_NAME	<Outer Layers>
{
WIDTH	6
GAP	6
}
}
}
}

*FIELDS*    USER FIELDS

"Drawn By" 
"Checked By" 
"QC By" 
"Released By" 
"Drawn Date" 2025-11-29
"Checked Date" 
"QC Date" 
"Release Date" 
"Company Name" Nations
"TITLE" N32A052KBQX_STB
"CODE" 
"Drawing Number" 
"Revision" V1.0
"SCALE" 
"DRAWN" 
"CHECKED" 
"QUALITY CONTROL" 
"RELEASED" 
"COMPANY" 
"COMPANY ADDRESS" 
"DRAWING NO" 
"REV" 

*SHT*   1 NS-LINK -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        5.866          Scale of window expansion
WINDOWCENTER 4518   2286    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

2550   7150   0   1 222  10 0 "Regular Arial Unicode MS"
DEBUG USB
8000   1940   0   1 222  10 0 "Regular Arial Unicode MS"
HEADER
2250   4050   0   1 222  10 0 "Regular Arial Unicode MS"
LED
4850   7150   0   1 222  10 0 "Regular Arial Unicode MS"
MCU
6100   7550   0   1 222  10 0 "Regular Arial Unicode MS"
NS-LINK
3778   1906   0   1 222  10 0 "Regular Arial Unicode MS"
3.3 TO 5V

*LINES*      LINES ITEMS

DRW20918         LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1200  232    0   0 97   10 1 "Regular Arial Unicode MS"
TITLE
-1202  -110   0   0 97   10 1 "Regular Arial Unicode MS"
Drawn Date
-300   42     0   0 97   10 1 "Regular Arial Unicode MS"
Revision
50     774    0   0 250  25 0 "Regular Arial Unicode MS"
A
50     2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
50     4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
50     6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-896   7400   0   0 250  25 0 "Regular Arial Unicode MS"
1
-2680  7400   0   0 250  25 0 "Regular Arial Unicode MS"
2
-4526  7400   0   0 250  25 0 "Regular Arial Unicode MS"
3
-6246  7400   0   0 250  25 0 "Regular Arial Unicode MS"
4
-8026  7400   0   0 250  25 0 "Regular Arial Unicode MS"
5
-9810  7400   0   0 250  25 0 "Regular Arial Unicode MS"
6
-1560  42     0   0 97   10 0 "Regular Arial Unicode MS"
SIZE:
-1560  -110   0   0 97   10 0 "Regular Arial Unicode MS"
DATED:
-10900 2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
-10900 774    0   0 250  25 0 "Regular Arial Unicode MS"
A
-10900 4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
-10900 6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-1102  42     0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Size
-118   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Number of Sheets
-320   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Number
-630   -110   0   0 97   10 0 "Regular Arial Unicode MS"
SHEET:     OF
-630   42     0   0 97   10 0 "Regular Arial Unicode MS"
REV:
-1560  232    0   0 97   10 0 "Regular Arial Unicode MS"
TITLE:
D25057           LINES    3300   7400   1   0
CLOSED 5   10  0  
0      0     
0      -5100 
7400   -5100 
7400   0     
0      0     
D25058           LINES    700    7400   1   0
CLOSED 5   10  0  
0      0     
0      -2900 
2500   -2900 
2500   0     
0      0     
D25059           LINES    700    2200   1   0
CLOSED 5   10  0  
0      0     
0      -1600 
5750   -1600 
5750   0     
0      0     
D25060           LINES    700    4400   1   0
CLOSED 5   10  0  
0      0     
0      -2100 
2500   -2100 
2500   0     
0      0     
DRW26078         LINES    600    7800   1   0
OPEN   8   10  0  
0      0     
0      -7300 
8800   -7300 
8800   -5600 
10200  -5600 
10200  0     
0      0     
0      -100  
D73140           LINES    6600   2200   1   0
CLOSED 5   10  0  
0      0     
0      -1600 
2600   -1600 
2600   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

PIN150           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2019.06.10.07.24.17
"Regular default"
"Regular default"
50 600 0 8 93 10 "Regular default"
REF-DES
-50 600 0 1 93 10 "Regular default"
PART-TYPE
OPEN   2   1   255
0     0    
-300  0    

PIN50            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 1970.01.01.00.00.00
"Default Font"
"Default Font"
-320 300 0 8 107 10 "Default Font"
REF-DES
-550 300 0 1 107 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-100  0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CON_MINIUSB      32000 32000 100 10 100 10 4 1 0 11 0 0
TIMESTAMP 2019.12.11.09.21.40
"Default Font"
"Default Font"
80 1260 0 4 100 10 "Default Font"
REF-DES
290 -40 0 6 100 10 "Default Font"
PART-TYPE
340 -150 0 6 100 10 "Default Font"
*
350 -270 0 6 100 10 "Default Font"
*
OPEN   5   10  255
0     0    
0     1200 
500   1200 
500   0    
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CON-SIP-4P       32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.11.27.05.40.08
"Default Font"
"Default Font"
50 50 0 4 97 10 "Default Font"
REF-DES
100 -500 0 6 97 10 "Default Font"
PART-TYPE
100 -600 0 6 97 10 "Default Font"
*
100 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -500 
200   -500 
200   0    
0     0    
T-100  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -200  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -300  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -400  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

N32G4XC          32000 32000 97 10 97 10 4 1 0 48 0 0
TIMESTAMP 2019.11.28.08.56.49
"Default Font"
"Default Font"
2300 2340 0 0 97 10 "Default Font"
REF-DES
2300 -40 0 2 97 10 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 "Default Font"
*
2300 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2300  0    
2300  2300 
0     2300 
0     0    
T-200  1700  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1700  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.28
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CON1X3           32000 32000 100 10 100 10 4 7 0 3 0 0
TIMESTAMP 2019.12.01.16.15.06
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 -250 0 6 100 10 "Default Font"
PART-TYPE
0 -240 0 6 100 10 "Default Font"
*
0 -340 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
0     50   
0     150  
CIRCLE 2   10  255
0     -50  
0     50   
CLOSED 5   10  255
-100  200  
-100  -200 
100   -200 
100   200  
-100  200  
CIRCLE 2   10  255
0     -50  
0     -150 
OPEN   2   10  255
-100  100  
-50   100  
OPEN   2   10  255
-100  -100 
-50   -100 
OPEN   2   10  255
-50   0    
-100  0    
T-200  100   0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAP00402         32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2025.07.22.08.10.31
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CAP0603          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2025.07.22.08.23.54
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

TXS0104EPWR      32000 32000 100 10 100 10 2 3 0 14 3 0
TIMESTAMP 1970.01.01.00.00.00
"Default Font"
"Default Font"
0 0 0 0 100 10 "Regular default"
REF-DES
0 0 0 0 100 10 "Default Font"
PART-TYPE
CIRCLE 2   10  255
-360  370  
-340  370  
CIRCLE 2   10  255
-360  370  
-340  370  
CLOSED 5   10  255
-400  -420 
-400  420  
400   420  
400   -420 
-400  -420 
T-500  300   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  200   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  100   0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  0     0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -100  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -200  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T-500  -300  0 1 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -300  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -200  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   -100  0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   0     0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   100   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   200   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0
T500   300   0 0 50 0 0 0 -180 0 0 9 PIN50
P0 0 0 0 0 0 0 0 0

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2019.11.20.07.32.26
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

RES              32000 32000 100 10 100 10 4 1 0 2 26 0
TIMESTAMP 2023.10.19.06.35.11
"Default Font"
"Default Font"
0 0 0 4 70 7 "Default Font"
REF-DES
240 -110 0 6 70 7 "Default Font"
PART-TYPE
150 30 0 6 70 7 "Default Font"
VALUE
210 -170 0 6 70 7 "Default Font"
*
CLOSED 5   10  255
50    -40  
50    40   
250   40   
250   -40  
50    -40  
T0     0     0 0 20 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T300   0     0 1 0 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

MINIUSB CON  1   0   0     0
TIMESTAMP 2019.12.11.09.21.39
GATE 1 11 0
CON_MINIUSB
1 0 U VBUS
2 0 U D-
3 0 U D+
4 0 U ID
5 0 U GND
6 0 U SHIELD1
7 0 U SHIELD2
8 0 U SHIELD3
9 0 U SHIELD4
10 0 U H1
11 0 U H2

CON-SIP-4P CON  1   0   0     0
TIMESTAMP 2019.11.27.05.40.07
GATE 1 4 0
CON-SIP-4P
1 0 U
2 0 U
3 0 U
4 0 U

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

N32G4XC UND  1   0   0     0
TIMESTAMP 2019.11.28.08.56.48
GATE 1 48 0
N32G4XC
1 0 U VBAT
2 0 U PC13-TAMPER-RTC
3 0 U PC14-OSC32_IN
4 0 U PC15-OSC32_OUT
5 0 U PD0-OSC_IN
6 0 U PD1-OSC_OUT
7 0 U NRST
8 0 U VSSA
9 0 U VDDA
10 0 U PA0-WKUP
11 0 U PA1
12 0 U PA2
13 0 U PA3
14 0 U PA4
15 0 U PA5
16 0 U PA6
17 0 U PA7
18 0 U PB0
19 0 U PB1
20 0 U PB2-BOOT
21 0 U PB10
22 0 U PB11
23 0 U VSS_1
24 0 U VDD_1
25 0 U PB12
26 0 U PB13
27 0 U PB14
28 0 U PB15
29 0 U PA8
30 0 U PA9
31 0 U PA10
32 0 U PA11
33 0 U PA12
34 0 U PA13-SWDIO
35 0 U VSS_2
36 0 U VDD_2
37 0 U PA14-SWCLK
38 0 U PA15
39 0 U PB3
40 0 U PB4
41 0 U PB5
42 0 U PB6
43 0 U PB7
44 0 U BOOT0
45 0 U PB8
46 0 U PB9
47 0 U VSS_3
48 0 U VDD_3

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

CON1X3 CON  1   0   0     3
TIMESTAMP 2019.12.01.16.15.04
GATE 1 3 0
CON1X3
1 0 U
2 0 U
3 0 U
1 2 3 

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U

C0402 CAP  1   0   0     0
TIMESTAMP 2025.07.22.08.10.29
GATE 1 2 0
CAP00402
1 1 U
2 1 U

C0603 CAP  1   0   0     0
TIMESTAMP 2025.07.22.08.23.51
GATE 1 2 0
CAP0603
1 1 U
2 1 U

TXS0104EPWR TTL  1   0   0     0
TIMESTAMP 1970.01.01.00.00.00
GATE 1 14 0
TXS0104EPWR
1 0 L VCCA
2 0 L A1
3 0 L A2
4 0 L A3
5 0 L A4
6 0 L NC
7 0 L GND
8 0 L OE
9 0 L NC
10 0 L B4
11 0 L B3
12 0 L B2
13 0 L B1
14 0 L VCCB

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2019.11.20.07.32.25
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

RES0402-4.7K RES  1   0   0     0
TIMESTAMP 2012.09.11.08.57.54
GATE 1 2 0
RES
1 0 U
2 0 U



*PART*       ITEMS



J4           MINIUSB          1350  5150    0 1 97 10 97 10 4 3 11 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 1300 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
290 -40 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
340 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
350 -270 0 6 97 10 0 "Regular Arial Unicode MS"
*
"DECAL" 
"Description" 6 pin header
"PCB DECAL" CON_MINIUSB
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1

J10          CON-SIP-4P       8500  1600    0 0 97 10 97 10 4 1 4 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 50 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
100 -500 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -600 0 6 97 10 0 "Regular Arial Unicode MS"
*
100 -700 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SIP-4P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1
3 60 10 0 1

R20          R0402            2750  3650    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 0 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R15          R0402            2750  3050    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 0 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D6           LED0805          1850  3700    0 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
300 -200 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D7           LED0805          1850  3100    0 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
300 -200 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

R11          R0402            1850  6100    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 100 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R12          R0402            1850  6000    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 -50 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 100 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C22          CAP1206          1800  6850    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
40 -170 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
40 -310 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

U4           N32G4XC          6400  3400    0 0 97 10 97 10 4 2 48 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
1162 1258 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
950 1050 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
954 1162 0 2 97 10 1 "Regular Arial Unicode MS"
Value
2300 -240 0 2 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" QFP48-3
"Value" N32G455CCL7
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

C30          0402C            4250  5400    0 0 97 10 97 10 3 22 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 90 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
10 -80 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
10 -160 0 6 97 7 3 "Regular Arial Unicode MS"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C32          0402C            4250  4600    0 0 97 10 97 10 3 22 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 90 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
10 -80 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
10 -160 0 6 97 7 3 "Regular Arial Unicode MS"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

R19          R0402            9000  4050    0 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 128 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
336 144 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 100R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R17          R0402            7650  2750   90 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
206 -80 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
16 -92 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R4           R0402            4750  4050    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -10 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R18          R0402            7350  6400   90 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 -50 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -50 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C5           C0402            5350  5350    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

R24          R0402            6050  4150    0 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 0 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J12          CON1X3           5900  6900    0 1 97 10 97 10 4 2 3 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 250 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -250 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -240 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -340 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Marking" 
"PCB DECAL" 2.54MM_CON3P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1

Y1           CRYSTAL_2PIN     4700  5250   90 3 97 10 97 10 4 2 2 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 -200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
260 -120 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
350 -200 90 5 97 10 1 "Regular Arial Unicode MS"
Value
240 -396 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Value" 8MHz
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1

C4           C0402            6300  6300    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

C6           C0402            9200  5600    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

C1           C0402            5000  3900    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

C8           C0402            5500  4200    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

C9           C0402            8300  3100    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
68 -128 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
68 -334 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0402
0 20 -90 0 0
1 20 -80 0 0

C14          C0603            6000  5800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
64 -420 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
52 -62 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" CAP0603
0 20 -90 0 0
1 20 -80 0 0

U3           TXS0104EPWR      3400  1300    0 0 97 10 97 10 23 22 14 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-54 -524 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
-302 -654 0 0 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Comment
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Symbol
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Device
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
LCSC_Part_Name
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier_Part
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Manufacturer
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Manufacturer_Part
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier_Footprint
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
JLCPCB_Part_Class
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Datasheet
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Supplier
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Add_into_BOM
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Convert_to_PCB
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Channel_Type
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Data_Rate
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Voltage___Supply(VCCA)
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Voltage___Supply(VCCB)
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Number_of_Circuits
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Output_Type
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Operating_Temperature
0 0 0 0 97 10 0 "Regular Arial Unicode MS"
Features
"Comment" TXS0104EPWR
"Symbol" TXS0104EPWR
"Device" TXS0104EPWR
"LCSC_Part_Name" TXS0104EPWR
"Supplier_Part" C44955
"Manufacturer" 
"Manufacturer_Part" TXS0104EPWR
"Supplier_Footprint" TSSOP-14
"JLCPCB_Part_Class" Extended Part
"Datasheet" https://www.ti.com/cn/lit/gpn/txs0104e
"Supplier" LCSC
"Add_into_BOM" yes
"Convert_to_PCB" yes
"Channel_Type" 
"Data_Rate" 24Mbps
"Voltage___Supply(VCCA)" 1.65V~3.6V
"Voltage___Supply(VCCB)" 2.3V~5.5V
"Number_of_Circuits" 4
"Output_Type" 
"Operating_Temperature" 
"Features" 
"PCB DECAL" TSSOP-14_L5.0-W4.4-P0.65-LS6.4-BL
0 50 0 0 0
1 50 0 0 0
2 50 0 0 0
3 50 0 0 0
4 50 0 0 0
5 50 0 0 0
6 50 0 0 0
7 50 0 0 0
8 50 0 0 0
9 50 0 0 0
10 50 0 0 0
11 50 0 0 0
12 50 0 0 0
13 50 0 0 0

J19          CONDIP2_A        4650  1500   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J20          CONDIP2_A        4650  1400   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J21          CONDIP2_A        4650  1300   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J22          CONDIP2_A        4650  1200   90 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R22          RES0402-4.7K     4504  998     0 1 97 10 97 10 4 7 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
222 -154 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
240 -110 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
-6 -90 0 6 97 7 3 "Regular Arial Unicode MS"
Value
210 -170 0 6 97 7 0 "Regular Arial Unicode MS"
*
"Code" 045020100277
"Description" RC0402FR-074K7L(4.7k¦¸,¡À1%,1/16W,SMD0402,YAGEO)
"Manufacturer" YAGEO
"PACKAGE" RES0402
"Part Number" RC0402FR-074K7L
"Value" 4.7K
"PCB DECAL" RES0402
0 20 20 0 0
1 0 20 0 0

J5           CONDIP2_A        6850  2750   90 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-140 -10 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 1800   6850   0 3 0
@@@O1    DP_NSLINK $OSR_SYMS 2350   6050   0 1 0
@@@O2    DM_NSLINK $OSR_SYMS 2350   6150   0 1 0
@@@O3    GND $GND_SYMS 1750   5450   0 0 0
@@@O4    GND $GND_SYMS 3000   3050   0 0 0
@@@O5    LED_CON/PB6 $OSR_SYMS 1750   3700   0 0 0
@@@O6    LED_RUN/PA8 $OSR_SYMS 1750   3100   0 0 0
@@@O7    5V $PWR_SYMS 2750   6450   0 0 0
@@@O8    VDD_LINK $PWR_SYMS 8250   1600   0 0 0
@@@O9    PA13/TMS/SWDIO $OSR_SYMS 8200   1400   0 0 0
@@@O10   PA14/TCK/SWCLK $OSR_SYMS 8200   1300   0 0 0
@@@O11   GND $GND_SYMS 8250   1150   0 0 0
@@@O12   VDD_LINK $PWR_SYMS 4300   4100   90 0 0
@@@O13   GND $GND_SYMS 5000   3350   0 0 0
@@@O14   DM_NSLINK $OSR_SYMS 9450   4700   0 1 0
@@@O15   DP_NSLINK $OSR_SYMS 9450   4800   0 1 0
@@@O16   PA14/TCK/SWCLK $OSR_SYMS 8100   6000   90 2 0
@@@O17   PA13/TMS/SWDIO $OSR_SYMS 9450   4900   0 1 0
@@@O18   LED_RUN/PA8 $OSR_SYMS 9450   4400   0 1 0
@@@O19   LED_CON/PB6 $OSR_SYMS 7600   6000   90 2 0
@@@O20   GND $GND_SYMS 7700   2600   0 0 0
@@@O21   VDD_LINK $PWR_SYMS 5600   5800   0 0 0
@@@O22   VDD_LINK $PWR_SYMS 7000   6450   0 0 0
@@@O23   VDD_LINK $PWR_SYMS 9000   5800   0 0 0
@@@O24   GND $GND_SYMS 9250   5000   90 0 0
@@@O25   GND $GND_SYMS 7100   6100   0 2 0
@@@O26   GND $GND_SYMS 8000   3000   0 0 0
@@@O27   VDD_LINK $PWR_SYMS 8550   3100   90 1 0
@@@O28   NSLINK_TCK_SWCLK $OSR_SYMS 9450   4100   0 1 0
@@@O29   NSLINK_TMS_SWDIO $OSR_SYMS 9450   4200   0 1 0
@@@O30   GND $GND_SYMS 4050   4600   90 1 0
@@@O31   GND $GND_SYMS 4050   5400   90 1 0
@@@O32   GND $GND_SYMS 6200   4400   90 1 0
@@@O33   VDD_LINK $PWR_SYMS 6150   7000   90 1 0
@@@O34   GND $GND_SYMS 6200   6800   90 0 0
@@@O35   NSLINK_USART1_RX $OSR_SYMS 9450   4600   0 1 0
@@@O36   NSLINK_USART1_TX $OSR_SYMS 9450   4500   0 1 0
@@@O37   GND $GND_SYMS 6200   5700   0 0 0
@@@O38   GND $GND_SYMS 5350   4900   0 0 0
@@@O39   GND $GND_SYMS 5500   3450   0 0 0
@@@O40   GND $GND_SYMS 8300   2600   0 0 0
@@@O41   VDD_LINK $PWR_SYMS 2400   1800   0 0 0
@@@O42   VDD_MCU $PWR_SYMS 4450   1800   0 0 0
@@@O43   NSLINK_USART1_RX $OSR_SYMS 2000   1500   0 0 0
@@@O44   NSLINK_USART1_TX $OSR_SYMS 2000   1400   0 0 0
@@@O45   NSLINK_TMS_SWDIO $OSR_SYMS 2000   1300   0 0 0
@@@O46   NSLINK_TCK_SWCLK $OSR_SYMS 2000   1200   0 0 0
@@@O47   MCU_PA9/TX $OSR_SYMS 5100   1500   0 1 0
@@@O48   MCU_PA10/RX $OSR_SYMS 5100   1400   0 1 0
@@@O49   PA13/SWDIO $OSR_SYMS 5100   1300   0 1 0
@@@O50   PA14/SWDCK $OSR_SYMS 5100   1200   0 1 0
@@@O51   GND $GND_SYMS 2600   950    0 0 0
@@@O52   VDD_LINK $PWR_SYMS 4682   998    90 1 0
@@@O53   NRST $OSR_SYMS 6500   2750   0 0 0

*TIEDOTS*



@@@D0    1750   5750  
@@@D1    1750   5650  
@@@D2    1750   5550  
@@@D3    1750   5450  
@@@D4    1800   6350  
@@@D5    3000   3100  
@@@D6    5000   4100  
@@@D7    9350   4200  
@@@D8    4700   5400  
@@@D9    4700   4600  
@@@D10   5600   4300  
@@@D11   5600   5100  
@@@D12   6200   5700  
@@@D13   7000   6400  
@@@D14   6300   6400  
@@@D15   5600   5550  
@@@D16   5600   4300  
@@@D17   9000   5700  
@@@D18   9200   5000  
@@@D19   8300   3100  

*CONNECTION*


*SIGNAL* $$$28647 64 0
J22.2        U3.10        2 0
4450   1200  
3900   1200  

*SIGNAL* $$$28650 64 0
U3.11        J21.2        2 0
3900   1300  
4450   1300  

*SIGNAL* $$$28651 64 0
U3.12        J20.2        2 0
3900   1400  
4450   1400  

*SIGNAL* $$$28652 64 0
U3.13        J19.2        2 0
3900   1500  
4450   1500  

*SIGNAL* MCU_PA10/RX 0 0
J20.1        @@@O48       2 0
4850   1400  
5100   1400  

*SIGNAL* $$$32065 64 0
U3.8         R22.2        3 0
3900   1000  
4204   1000  
4204   998   

*SIGNAL* MCU_PA9/TX 0 0
J19.1        @@@O47       2 0
4850   1500  
5100   1500  

*SIGNAL* $$$11285 64 0
U4.18        J5.2         3 0
7500   3200  
7500   2750  
7050   2750  

*SIGNAL* PA13/SWDIO 0 0
J21.1        @@@O49       2 0
4850   1300  
5100   1300  

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
U3.14        @@@O42       3 0
3900   1600  
4450   1600  
4450   1800  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        C22.1        2 0
1800   6850  
1800   6850  
J4.5         @@@D0        3 0
1550   5850  
1750   5850  
1750   5750  
J4.6         @@@D0        2 0
1550   5750  
1750   5750  
@@@D0        @@@D1        2 0
1750   5750  
1750   5650  
J4.7         @@@D1        2 0
1550   5650  
1750   5650  
@@@D1        @@@D2        2 0
1750   5650  
1750   5550  
J4.8         @@@D2        2 0
1550   5550  
1750   5550  
@@@D2        @@@D3        2 0
1750   5550  
1750   5450  
J4.9         @@@D3        2 0
1550   5450  
1750   5450  
@@@D3        @@@O3        2 0
1750   5450  
1750   5450  
@@@D5        R20.1        3 0
3000   3100  
3000   3700  
2850   3700  
@@@D5        R15.1        2 0
3000   3100  
2850   3100  
@@@D5        @@@O4        2 0
3000   3100  
3000   3050  
J10.4        @@@O11       3 0
8400   1200  
8250   1200  
8250   1150  
C1.2         @@@O13       2 0
5000   3400  
5000   3350  
@@@O20       R17.1        2 0
7700   2600  
7700   2650  
U4.35        @@@D18       2 0
8900   5000  
9200   5000  
U4.47        @@@O25       2 0
7100   5900  
7100   6100  
@@@O30       C32.1        2 0
4050   4600  
4150   4600  
C30.1        @@@O31       2 0
4150   5400  
4050   5400  
U4.8         @@@O32       2 0
6200   4400  
6200   4400  
U4.23        @@@O26       2 0
8000   3200  
8000   3000  
J12.3        @@@O34       2 0
6100   6800  
6200   6800  
C4.2         @@@D12       3 0
6300   5800  
6300   5700  
6200   5700  
@@@D12       C14.1        3 0
6200   5700  
6000   5700  
6000   5800  
@@@D12       @@@O37       2 0
6200   5700  
6200   5700  
C5.2         @@@O38       2 0
5350   4850  
5350   4900  
C8.2         @@@O39       2 0
5500   3700  
5500   3450  
C9.2         @@@O40       2 0
8300   2600  
8300   2600  
C6.2         @@@D18       2 0
9200   5100  
9200   5000  
@@@D18       @@@O24       2 0
9200   5000  
9250   5000  
U3.7         @@@O51       3 0
2900   1000  
2600   1000  
2600   950   

*SIGNAL* 5V 0 0
C22.2        @@@D4        2 0
1800   6350  
1800   6350  
@@@D4        J4.1         3 0
1800   6350  
1800   6250  
1550   6250  
@@@O7        @@@D4        4 0
2750   6450  
2750   6400  
1800   6400  
1800   6350  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J10.1        @@@O8        3 0
8400   1500  
8250   1500  
8250   1600  
@@@O12       R4.2         2 0
4300   4100  
4450   4100  
U4.9         @@@D10       2 0
6200   4300  
5600   4300  
@@@O21       @@@D15       2 0
5600   5800  
5600   5550  
@@@O22       @@@D13       2 0
7000   6450  
7000   6400  
@@@D17       @@@O23       2 0
9000   5700  
9000   5800  
@@@D10       R24.2        3 0
5600   4300  
5600   4200  
5750   4200  
@@@D11       @@@D16       2 0
5600   5100  
5600   4300  
@@@D11       U4.1         2 0
5600   5100  
6200   5100  
J12.1        @@@O33       2 0
6100   7000  
6150   7000  
@@@D13       @@@D14       2 0
7000   6400  
6300   6400  
C4.1         @@@D14       2 0
6300   6300  
6300   6400  
@@@D13       U4.48        2 0
7000   6400  
7000   5900  
@@@D14       C14.2        3 0
6300   6400  
6000   6400  
6000   6300  
C5.1         @@@D15       3 0
5350   5350  
5350   5550  
5600   5550  
@@@D15       @@@D11       2 0
5600   5550  
5600   5100  
C8.1         @@@D16       3 0
5500   4200  
5500   4300  
5600   4300  
@@@D16       @@@D10       2 0
5600   4300  
5600   4300  
@@@O27       @@@D19       2 0
8550   3100  
8300   3100  
@@@D17       U4.36        3 0
9000   5700  
9000   5100  
8900   5100  
@@@D17       C6.1         3 0
9000   5700  
9200   5700  
9200   5600  
C9.1         @@@D19       2 0
8300   3100  
8300   3100  
@@@D19       U4.24        3 0
8300   3100  
8100   3100  
8100   3200  
U3.1         @@@O41       3 0
2900   1600  
2400   1600  
2400   1800  
R22.1        @@@O52       2 0
4504   998   
4682   998   

*SIGNAL* NRST 0 0
J5.1         @@@O53       2 0
6650   2750  
6500   2750  

*SIGNAL* DM_NSLINK 0 0
R11.2        @@@O2        2 0
2150   6150  
2350   6150  
U4.32        @@@O14       2 0
8900   4700  
9450   4700  

*SIGNAL* DP_NSLINK 0 0
R12.2        @@@O1        2 0
2150   6050  
2350   6050  
U4.33        @@@O15       2 0
8900   4800  
9450   4800  

*SIGNAL* $$$24935 64 0
J4.2         R11.1        2 0
1550   6150  
1750   6150  

*SIGNAL* $$$24997 64 0
J4.3         R12.1        2 0
1550   6050  
1750   6050  

*SIGNAL* $$$32273 64 0
D6.1         R20.2        2 0
2350   3700  
2450   3700  

*SIGNAL* $$$32275 64 0
D7.1         R15.2        2 0
2350   3100  
2450   3100  

*SIGNAL* LED_CON/PB6 0 0
D6.2         @@@O5        2 0
1850   3700  
1750   3700  
U4.42        @@@O19       2 0
7600   5900  
7600   6000  

*SIGNAL* LED_RUN/PA8 0 0
D7.2         @@@O6        2 0
1850   3100  
1750   3100  
@@@O18       U4.29        2 0
9450   4400  
8900   4400  

*SIGNAL* PA13/TMS/SWDIO 0 0
J10.2        @@@O9        2 0
8400   1400  
8200   1400  
U4.34        @@@O17       2 0
8900   4900  
9450   4900  

*SIGNAL* PA14/TCK/SWCLK 0 0
J10.3        @@@O10       2 0
8400   1300  
8200   1300  
U4.37        @@@O16       2 0
8100   5900  
8100   6000  

*SIGNAL* NSLINK_TMS_SWDIO 0 0
@@@D7        U4.27        2 0
9350   4200  
8900   4200  
R19.2        @@@D7        3 0
9300   4000  
9350   4000  
9350   4200  
@@@D7        @@@O29       2 0
9350   4200  
9450   4200  
@@@O45       U3.4         2 0
2000   1300  
2900   1300  

*SIGNAL* NSLINK_TCK_SWCLK 0 0
@@@O28       U4.26        2 0
9450   4100  
8900   4100  
U3.5         @@@O46       2 0
2900   1200  
2000   1200  

*SIGNAL* NSLINK_USART1_TX 0 0
U4.30        @@@O36       2 0
8900   4500  
9450   4500  
@@@O44       U3.3         2 0
2000   1400  
2900   1400  

*SIGNAL* NSLINK_USART1_RX 0 0
U4.31        @@@O35       2 0
8900   4600  
9450   4600  
@@@O43       U3.2         2 0
2000   1500  
2900   1500  

*SIGNAL* $$$14362 64 0
R4.1         @@@D6        2 0
4850   4100  
5000   4100  
@@@D6        U4.7         4 0
5000   4100  
5300   4100  
5300   4500  
6200   4500  
@@@D6        C1.1         2 0
5000   4100  
5000   3900  

*SIGNAL* $$$32474 64 0
R17.2        U4.20        2 0
7700   3050  
7700   3200  

*SIGNAL* $$$32494 64 0
U4.44        R18.1        2 0
7400   5900  
7400   6300  

*SIGNAL* $$$29264 64 0
R18.2        J12.2        3 0
7400   6700  
7400   6900  
6100   6900  

*SIGNAL* $$$18547 64 0
U4.25        R19.1        2 0
8900   4000  
8900   4000  

*SIGNAL* $$$26932 64 0
Y1.2         @@@D9        2 0
4700   4698  
4700   4600  
U4.6         @@@D9        2 0
6200   4600  
4700   4600  
@@@D9        C32.2        2 0
4700   4600  
4350   4600  

*SIGNAL* $$$26931 64 0
Y1.1         @@@D8        2 0
4700   5298  
4700   5400  
U4.5         @@@D8        4 0
6200   4700  
5100   4700  
5100   5400  
4700   5400  
@@@D8        C30.2        2 0
4700   5400  
4350   5400  

*SIGNAL* $$$3902 64 0
U4.10        R24.1        2 0
6200   4200  
6150   4200  

*SIGNAL* PA14/SWDCK 0 0
J22.1        @@@O50       2 0
4850   1200  
5100   1200  

*NETNAMES*



DP_NSLINK    @@@O1        320    -40    0 0 0      0      0 3 -1 12 97 "Regular Arial Unicode MS"
DM_NSLINK    @@@O2        322    -32    0 0 0      0      0 3 -1 12 97 "Regular Arial Unicode MS"
LED_CON/PB6  @@@O5        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_RUN/PA8  @@@O6        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
5V           @@@O7        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O8        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA13/TMS/SWDIO @@@O9        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/TCK/SWCLK @@@O10       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O12       -400   0      0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
DM_NSLINK    @@@O14       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
DP_NSLINK    @@@O15       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/TCK/SWCLK @@@O16       -50    950    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA13/TMS/SWDIO @@@O17       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_RUN/PA8  @@@O18       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
LED_CON/PB6  @@@O19       -50    850    90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O21       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O22       -300   100    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O23       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O27       400    50     0 7 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TCK_SWCLK @@@O28       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TMS_SWDIO @@@O29       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O33       400    0      0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_RX @@@O35       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_TX @@@O36       360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O41       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O42       0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_RX @@@O43       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_USART1_TX @@@O44       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TMS_SWDIO @@@O45       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
NSLINK_TCK_SWCLK @@@O46       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA9/TX   @@@O47       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA10/RX  @@@O48       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13/SWDIO   @@@O49       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/SWDCK   @@@O50       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O52       420    -42    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NRST         @@@O53       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Tahoma"

*SHT*   2 MCU -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        9.844          Scale of window expansion
WINDOWCENTER 4271   921     Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

9736   4324   0   0 222  10 0 "Regular Arial Unicode MS"
RESET
7700   7508   0   1 222  10 0 "Regular Arial Unicode MS"
KEY
10198  7506   0   1 222  10 0 "Regular Arial Unicode MS"
LED
2904   7558   0   1 222  10 0 "Regular Arial Unicode MS"
LDO
1934   5364   0   1 222  10 0 "Regular Arial Unicode MS"
MCU
8578   1954   0   1 278  10 0 "Regular Arial Unicode MS"
8M Crystal
7320   4324   0   0 222  10 0 "Regular Arial Unicode MS"
MCU WAKEUP

*LINES*      LINES ITEMS

DRW_NATIONS_A4   LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1200  232    0   0 97   10 1 "Regular Arial Unicode MS"
TITLE
-1202  -110   0   0 97   10 1 "Regular Arial Unicode MS"
Drawn Date
-300   42     0   0 97   10 1 "Regular Arial Unicode MS"
Revision
-1560  232    0   0 97   10 0 "Regular Arial Unicode MS"
TITLE:
-630   42     0   0 97   10 0 "Regular Arial Unicode MS"
REV:
-630   -110   0   0 97   10 0 "Regular Arial Unicode MS"
SHEET:     OF
-320   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Number
-118   -110   0   0 97   10 1 "Regular Arial Unicode MS"
Number of Sheets
-1102  42     0   0 97   10 1 "Regular Arial Unicode MS"
Sheet Size
-10900 6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
-10900 4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
-10900 774    0   0 250  25 0 "Regular Arial Unicode MS"
A
-10900 2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
-1560  -110   0   0 97   10 0 "Regular Arial Unicode MS"
DATED:
-1560  42     0   0 97   10 0 "Regular Arial Unicode MS"
SIZE:
-9810  7400   0   0 250  25 0 "Regular Arial Unicode MS"
6
-8026  7400   0   0 250  25 0 "Regular Arial Unicode MS"
5
-6246  7400   0   0 250  25 0 "Regular Arial Unicode MS"
4
-4526  7400   0   0 250  25 0 "Regular Arial Unicode MS"
3
-2680  7400   0   0 250  25 0 "Regular Arial Unicode MS"
2
-896   7400   0   0 250  25 0 "Regular Arial Unicode MS"
1
50     6400   0   0 250  25 0 "Regular Arial Unicode MS"
D
50     4524   0   0 250  25 0 "Regular Arial Unicode MS"
C
50     2650   0   0 250  25 0 "Regular Arial Unicode MS"
B
50     774    0   0 250  25 0 "Regular Arial Unicode MS"
A
D22894           LINES    8850   4700   1   0
CLOSED 5   10  0  
0      0     
0      -2300 
2250   -2300 
2250   0     
0      0     
D23128           LINES    6700   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2050   -3000 
2050   0     
0      0     
D23129           LINES    8850   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2250   -3000 
2250   0     
0      0     
D24819           LINES    600    7800   1   0
CLOSED 5   10  0  
0      0     
0      -1900 
6000   -1900 
6000   0     
0      0     
DRW67184         LINES    600    5800   1   0
OPEN   9   10  0  
0      0     
0      -5300 
8900   -5300 
8900   -4300 
10500  -4300 
10500  -3500 
6000   -3500 
6000   0     
0      0     
D72668           LINES    6700   4700   1   0
CLOSED 5   10  0  
0      0     
0      -2300 
2050   -2300 
2050   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

PIN150           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2019.06.10.07.24.17
"Regular default"
"Regular default"
50 600 0 8 93 10 "Regular default"
REF-DES
-50 600 0 1 93 10 "Regular default"
PART-TYPE
OPEN   2   1   255
0     0    
-300  0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2020.05.30.04.20.05
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

SPX1117-3V3      32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.12.11.09.57.22
"Default Font"
"Default Font"
200 100 0 4 97 10 "Default Font"
REF-DES
200 -500 0 6 97 10 "Default Font"
PART-TYPE
200 -600 0 6 97 10 "Default Font"
*
200 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -400 
400   -400 
400   0    
0     0    
T-200  -300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

SW_2P            32000 32000 97 10 97 10 4 6 0 2 16 0
TIMESTAMP 2019.01.05.10.52.59
"Default Font"
"Default Font"
0 100 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
0 -200 0 6 97 10 "Default Font"
*
0 -300 0 6 97 10 "Default Font"
*
OPEN   2   20  255
-150  40   
150   40   
OPEN   2   30  255
-80   60   
80    60   
CIRCLE 2   10  255
-60   0    
-100  0    
CIRCLE 2   10  255
100   0    
60    0    
OPEN   2   10  255
80    0    
200   0    
OPEN   2   10  255
-80   0    
-200  0    
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T200   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CON1X3           32000 32000 100 10 100 10 4 7 0 3 0 0
TIMESTAMP 2019.12.01.16.15.06
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 -250 0 6 100 10 "Default Font"
PART-TYPE
0 -240 0 6 100 10 "Default Font"
*
0 -340 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
0     50   
0     150  
CIRCLE 2   10  255
0     -50  
0     50   
CLOSED 5   10  255
-100  200  
-100  -200 
100   -200 
100   200  
-100  200  
CIRCLE 2   10  255
0     -50  
0     -150 
OPEN   2   10  255
-100  100  
-50   100  
OPEN   2   10  255
-100  -100 
-50   -100 
OPEN   2   10  255
-50   0    
-100  0    
T-200  100   0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

HEAD2X14         32000 32000 97 10 97 10 4 1 0 28 0 0
TIMESTAMP 2025.07.22.07.04.35
"Default Font"
"Default Font"
200 1540 0 4 97 10 "Default Font"
REF-DES
100 -140 0 6 97 10 "Default Font"
PART-TYPE
100 -240 0 6 97 10 "Default Font"
*
100 -340 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
200   0    
200   1500 
0     1500 
0     0    
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAP0402          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2025.07.22.08.09.26
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CAP0603          32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2025.07.22.08.23.54
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

NS3611_QFN32     32000 32000 97 10 97 10 4 1 0 33 0 0
TIMESTAMP 2025.12.01.03.54.53
"Default Font"
"Default Font"
1900 1940 0 0 97 10 "Default Font"
REF-DES
1900 -40 0 2 97 10 "Default Font"
PART-TYPE
1900 -140 0 2 97 10 "Default Font"
*
1900 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
1500  0    
1500  1500 
0     1500 
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T300   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.42
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

RES              32000 32000 100 10 100 10 4 1 0 2 26 0
TIMESTAMP 2023.10.19.06.35.11
"Default Font"
"Default Font"
0 0 0 4 70 7 "Default Font"
REF-DES
240 -110 0 6 70 7 "Default Font"
PART-TYPE
150 30 0 6 70 7 "Default Font"
VALUE
210 -170 0 6 70 7 "Default Font"
*
CLOSED 5   10  255
50    -40  
50    40   
250   40   
250   -40  
50    -40  
T0     0     0 0 20 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T300   0     0 1 0 20 0 0 130 50 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2020.05.30.04.20.03
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

AMS1117-3.3 UND  1   0   0     0
TIMESTAMP 2019.12.11.09.57.22
GATE 1 4 0
SPX1117-3V3
1 0 U GND
2 0 U OUT
3 0 U IN
4 0 U OUT

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

SW_2P UND  1   0   0     2
TIMESTAMP 2019.01.05.10.52.56
GATE 1 2 0
SW_2P
1 0 U
2 0 U
1 2 

CON1X3 CON  1   0   0     3
TIMESTAMP 2019.12.01.16.15.04
GATE 1 3 0
CON1X3
1 0 U
2 0 U
3 0 U
1 2 3 

HEAD2X14 UND  1   0   0     0
TIMESTAMP 2025.07.22.07.04.35
GATE 1 28 0
HEAD2X14
1 0 L
2 0 L
3 0 L
4 0 L
5 0 L
6 0 L
7 0 L
8 0 L
9 0 L
10 0 L
11 0 L
12 0 L
13 0 L
14 0 L
15 0 L
16 0 L
17 0 L
18 0 L
19 0 L
20 0 L
21 0 U
22 0 U
23 0 U
24 0 U
25 0 U
26 0 U
27 0 U
28 0 U

CAP0402 CAP  1   0   0     0
TIMESTAMP 2025.07.22.08.09.25
GATE 1 2 0
CAP0402
1 1 U
2 1 U

C0603 CAP  1   0   0     0
TIMESTAMP 2025.07.22.08.23.51
GATE 1 2 0
CAP0603
1 1 U
2 1 U

N32G052KBQ7 UND  1   0   0     0
TIMESTAMP 2025.12.01.03.54.51
GATE 1 33 0
NS3611_QFN32
1 0 C PA12
2 0 C PA11-PC15
3 0 C NRST
4 0 C PD14-OSC_IN
5 0 C PD15-OSC_OUT
6 0 C VSS
7 0 C VDD
8 0 C PA0
9 0 C PA1
10 0 C PA2
11 0 C PB13
12 0 C PA3
13 0 C PA4-PA6
14 0 C PB0
15 0 C PB12
16 0 C PD0
17 0 C PA14
18 0 C PA13
19 0 C PB4
20 0 C PB8-PC10
21 0 C PC5
22 0 C PC6
23 0 C PC7
24 0 C PD11
25 0 C PD8
26 0 C PD5
27 0 C PD4
28 0 C PD12
29 0 C PD13
30 0 C PA9
31 0 C PA10
32 0 C PB3
33 0 C GND

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U

RES0201-0R RES  1   0   0     0
TIMESTAMP 2012.08.09.07.46.57
GATE 1 2 0
RES
1 0 U
2 0 U



*PART*       ITEMS



C31          CAP1206          3650  7050    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 -150 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
46 -352 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

C7           CAP1206          2000  7100    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
48 -172 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
240 -30 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
48 -338 0 2 97 10 3 "Regular Arial Unicode MS"
Value
180 -360 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

D4           LED0805          4500  7150   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 -100 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

U2           AMS1117-3.3      2950  7350    0 0 97 10 97 10 4 1 4 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
200 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
200 -500 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
200 -600 0 6 97 10 0 "Regular Arial Unicode MS"
*
200 -700 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SOT223
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1

R5           R0402            4550  6550   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S7           SW_2P            10450 3400    0 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 100 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R8           R0402            10150 3850   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D1           LED0805          9500  6250   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

S2           SW_2P            7300  6400   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R6           R0402            7350  6000   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S3           SW_2P            7700  6400   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R7           R0402            7750  6000   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S4           SW_2P            8100  6400   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R10          R0402            8150  6000   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R1           R0402            9550  5550   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J1           HEAD2X14         2150  700     0 0 97 10 97 10 4 1 28 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
102 1550 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
100 -140 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -240 0 6 97 10 0 "Regular Arial Unicode MS"
*
100 -340 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 2.54MM_CON2X14P
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1

U1           N32G052KBQ7      3000  3200    0 0 97 10 97 10 4 2 33 0 0 0
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
746 942 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
560 902 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
1900 -140 0 2 97 10 0 "Regular Arial Unicode MS"
*
1900 -240 0 2 97 10 0 "Regular Arial Unicode MS"
*
"VALUE" N32G4XXK
"PCB DECAL" NS-QFN32-50P500X500X80-J350X350
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1

J3           CON1X3           5150  7250    0 1 97 10 97 10 4 2 3 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 250 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -250 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -240 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -340 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Marking" 
"PCB DECAL" 2.54MM_CON3P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1

D2           LED0805          10050 6250   90 2 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

R23          R0402            10100 5550   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D3           LED0805          10550 5750   90 1 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
150 200 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
250 -150 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
250 -250 0 6 97 10 0 "Regular Arial Unicode MS"
*
250 -350 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

R13          R0402            1550  1850    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
302 68 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
292 34 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R14          R0402            2750  1850    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-114 66 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-114 28 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R16          R0402            1600  950     0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-114 66 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-114 28 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R21          R0402            2750  1050    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-114 66 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-114 28 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J2           HEAD2X14         5150  700     0 0 97 10 97 10 4 1 28 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
120 1542 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
100 -140 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
100 -240 0 6 97 10 0 "Regular Arial Unicode MS"
*
100 -340 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" 2.54MM_CON2X14P
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1

R26          R0402            5700  1750    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-114 66 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-114 28 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R27          R0402            4600  1750    0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
294 64 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
286 34 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R28          R0402            4600  950     0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
294 64 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
286 34 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R29          R0402            5700  950     0 0 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-92 64 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-100 40 0 6 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J9           CONDIP2_A        1700  7250   90 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-80 0 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

C12          CAP0402          2136  3138    0 2 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-178 -174 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-234 -352 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C13          CAP0402          10100 2800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-178 -174 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-234 -352 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C11          CAP0402          4000  6550    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-178 -174 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-234 -352 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

C2           CAP0402          2400  6600    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-178 -174 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-234 -352 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" CAP0402
0 20 -90 0 0
1 20 -80 0 0

S1           SW_2P            7950  3650   90 0 97 10 97 10 4 1 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
50 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
0 -200 0 6 97 10 0 "Regular Arial Unicode MS"
*
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R30          R0402            8000  3250   90 2 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J6           CONDIP2_A        9500  6550    0 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-140 -10 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J7           CONDIP2_A        10050 6550    0 1 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-130 -14 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J8           CONDIP2_A        10550 6550    0 2 97 10 97 10 4 3 2 0 0 18
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-124 -56 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -300 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-350 -50 0 6 97 10 0 "Regular Arial Unicode MS"
*
-350 -150 0 6 97 10 0 "Regular Arial Unicode MS"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R25          R0402            10500 5350   90 1 97 10 97 10 4 9 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
100 150 90 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
0 -100 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
150 150 90 5 97 10 1 "Regular Arial Unicode MS"
Value
80 -310 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C50          C0603            1786  3138    0 2 97 10 97 10 4 4 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
-228 -114 0 0 97 10 0 "Regular Arial Unicode MS"
REF-DES
210 -40 0 2 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
-296 -350 0 2 97 10 3 "Regular Arial Unicode MS"
Value
150 -340 0 2 97 10 0 "Regular Arial Unicode MS"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" CAP0603
0 20 -90 0 0
1 20 -80 0 0

C10          0402C            8446  1150   90 1 97 10 97 10 3 22 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 90 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
10 -80 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
10 -160 0 6 97 7 3 "Regular Arial Unicode MS"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C15          0402C            7646  1150   90 1 97 10 97 10 3 22 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
0 90 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
10 -80 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
10 -160 0 6 97 7 3 "Regular Arial Unicode MS"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

Y2           CRYSTAL_2PIN     8296  1450    0 3 97 10 97 10 4 2 2 0 0 2
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
250 120 0 4 97 10 0 "Regular Arial Unicode MS"
REF-DES
260 -120 0 6 97 10 0 "Regular Arial Unicode MS"
PART-TYPE
240 -296 0 6 97 10 0 "Regular Arial Unicode MS"
Value
240 -396 0 6 97 10 0 "Regular Arial Unicode MS"
*
"Value" 8MHz (AV08000301) 12pF
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1

R9           RES0201-0R       7250  1450    0 0 97 10 97 10 4 8 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
154 68 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
240 -110 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
150 20 0 6 97 7 3 "Regular Arial Unicode MS"
Value
210 -170 0 6 97 7 0 "Regular Arial Unicode MS"
*
"Code" 992070100125
"Description" RC0201JR-070RL(0¦¸,¡À5%,1/20W,SMD0201,YAGEO)
"Geometry.Height" 0.3mm
"Manufacturer" YAGEO
"PACKAGE" RES0201
"Part Number" RC0201JR-070RL
"Value" 0R
"PCB DECAL" RES0201
0 20 20 0 0
1 0 20 0 0

R31          RES0201-0R       8550  1450    0 0 97 10 97 10 4 8 2 0 0 26
"Regular Arial Unicode MS"
"Regular Arial Unicode MS"
154 68 0 4 97 7 0 "Regular Arial Unicode MS"
REF-DES
240 -110 0 6 97 7 0 "Regular Arial Unicode MS"
PART-TYPE
150 20 0 6 97 7 3 "Regular Arial Unicode MS"
Value
210 -170 0 6 97 7 0 "Regular Arial Unicode MS"
*
"Code" 992070100125
"Description" RC0201JR-070RL(0¦¸,¡À5%,1/20W,SMD0201,YAGEO)
"Geometry.Height" 0.3mm
"Manufacturer" YAGEO
"PACKAGE" RES0201
"Part Number" RC0201JR-070RL
"Value" 0R
"PCB DECAL" RES0201
0 20 20 0 0
1 0 20 0 0


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 2200   6300   0 0 0
@@@O1    GND $GND_SYMS 4500   6250   0 0 0
@@@O2    GND $GND_SYMS 3750   6250   0 0 0
@@@O3    GND $GND_SYMS 2750   6850   0 0 0
@@@O4    VDD_MCU $PWR_SYMS 5450   7250   90 1 0
@@@O5    5V $PWR_SYMS 1450   7300   0 0 0
@@@O6    VDD_LINK $PWR_SYMS 5450   6900   90 1 0
@@@O7    GND $GND_SYMS 10700  3250   0 0 0
@@@O8    GND $GND_SYMS 10100  2800   0 0 0
@@@O9    VDD_MCU $PWR_SYMS 10100  3950   0 0 0
@@@O10   PB0 $OSR_SYMS 9500   6900   90 2 0
@@@O11   GND $GND_SYMS 9500   5200   0 0 0
@@@O12   GND $GND_SYMS 7300   5550   0 0 0
@@@O13   GND $GND_SYMS 7700   5550   0 0 0
@@@O14   GND $GND_SYMS 8100   5550   0 0 0
@@@O15   PA1 $OSR_SYMS 7300   6800   90 2 0
@@@O16   PA2 $OSR_SYMS 7700   6800   90 2 0
@@@O17   PA3 $OSR_SYMS 8100   6800   90 2 0
@@@O18   VDD_MCU $PWR_SYMS 3100   2100   90 1 0
@@@O19   VDD_MCU $PWR_SYMS 1400   2100   90 0 0
@@@O20   PD14_OSC_IN $OSR_SYMS 2800   4000   0 0 0
@@@O21   PA2 $OSR_SYMS 3500   2900   90 0 0
@@@O22   PB13 $OSR_SYMS 3600   2900   90 0 0
@@@O23   PA3 $OSR_SYMS 3700   2900   90 0 0
@@@O24   PA4-PA6 $OSR_SYMS 3800   2900   90 0 0
@@@O25   PB0 $OSR_SYMS 3900   2900   90 0 0
@@@O26   PB12 $OSR_SYMS 4000   2900   90 0 0
@@@O27   PC6 $OSR_SYMS 4800   4100   0 1 0
@@@O28   PB8-PC10 $OSR_SYMS 4800   3900   0 1 0
@@@O29   PB4 $OSR_SYMS 4800   3800   0 1 0
@@@O30   PA13/SWDIO $OSR_SYMS 4800   3700   0 1 0
@@@O31   PC5 $OSR_SYMS 4800   4000   0 1 0
@@@O32   PC7 $OSR_SYMS 4800   4200   0 1 0
@@@O33   PD8 $OSR_SYMS 4100   4900   90 2 0
@@@O34   PD11 $OSR_SYMS 4800   4300   0 3 0
@@@O35   PD5 $OSR_SYMS 4000   4900   90 2 0
@@@O36   MCU_PA10/RX $OSR_SYMS 3500   4900   90 2 0
@@@O37   PD12 $OSR_SYMS 3800   4900   90 2 0
@@@O38   PD4 $OSR_SYMS 3900   4900   90 2 0
@@@O39   VDD_MCU $PWR_SYMS 1650   3700   90 0 0
@@@O40   GND $GND_SYMS 2136   3088   0 1 0
@@@O41   PD13 $OSR_SYMS 3700   4900   90 2 0
@@@O42   MCU_PA9/TX $OSR_SYMS 3600   4900   90 2 0
@@@O43   PA1 $OSR_SYMS 3400   2900   90 0 0
@@@O44   PA0 $OSR_SYMS 2800   3600   0 0 0
@@@O45   PD0_BOOT0 $OSR_SYMS 4100   2900   90 0 0
@@@O46   PB3 $OSR_SYMS 3400   4900   90 3 0
@@@O47   GND $GND_SYMS 3300   5030   90 3 0
@@@O48   NRST $OSR_SYMS 2800   4100   0 0 0
@@@O49   PA11-PC15 $OSR_SYMS 2800   4200   0 0 0
@@@O50   PB3 $OSR_SYMS 4850   1100   0 0 0
@@@O51   PD11 $OSR_SYMS 4850   1500   0 2 0
@@@O52   PB8-PC10 $OSR_SYMS 4850   1700   0 2 0
@@@O53   PD5 $OSR_SYMS 4850   1400   0 0 0
@@@O54   PD12 $OSR_SYMS 4850   1300   0 2 0
@@@O55   MCU_PA9/TX $OSR_SYMS 4850   1200   0 2 0
@@@O56   PC6 $OSR_SYMS 4850   1600   0 2 0
@@@O57   GND $GND_SYMS 4800   1900   90 1 0
@@@O58   PB4 $OSR_SYMS 5750   1700   0 1 0
@@@O59   PC5 $OSR_SYMS 5750   1600   0 3 0
@@@O60   PD8 $OSR_SYMS 5750   1400   0 3 0
@@@O61   PD4 $OSR_SYMS 5750   1300   0 3 0
@@@O62   PD13 $OSR_SYMS 5750   1200   0 3 0
@@@O63   PC7 $OSR_SYMS 5750   1500   0 3 0
@@@O64   MCU_PA10/RX $OSR_SYMS 5750   1100   0 3 0
@@@O65   GND $GND_SYMS 5700   1900   90 0 0
@@@O66   PB4 $OSR_SYMS 10050  6900   90 2 0
@@@O67   GND $GND_SYMS 10050  5200   0 0 0
@@@O68   PA11-PC15 $OSR_SYMS 1550   1700   0 0 0
@@@O69   PD0_BOOT0 $OSR_SYMS 1550   1800   0 0 0
@@@O70   PD15 $OSR_SYMS 1550   1600   0 0 0
@@@O71   PA1 $OSR_SYMS 1550   1500   0 0 0
@@@O72   PB13 $OSR_SYMS 1550   1400   0 0 0
@@@O73   PA4-PA6 $OSR_SYMS 1550   1300   0 0 0
@@@O74   PB12 $OSR_SYMS 1550   1200   0 0 0
@@@O75   PA13/SWDIO $OSR_SYMS 1550   1100   0 0 0
@@@O76   GND $GND_SYMS 1750   900    90 1 0
@@@O77   PA12 $OSR_SYMS 2850   1800   0 1 0
@@@O78   PA0 $OSR_SYMS 2850   1600   0 1 0
@@@O79   PA2 $OSR_SYMS 2850   1500   0 1 0
@@@O80   PA3 $OSR_SYMS 2850   1400   0 1 0
@@@O81   PB0 $OSR_SYMS 2850   1300   0 1 0
@@@O82   PA14/SWDCK $OSR_SYMS 2850   1200   0 1 0
@@@O83   PD14 $OSR_SYMS 2850   1700   0 1 0
@@@O84   GND $GND_SYMS 2700   1000   90 0 0
@@@O85   GND $GND_SYMS 2700   900    90 0 0
@@@O86   VDD_MCU $PWR_SYMS 1400   2000   90 0 0
@@@O87   VDD_MCU $PWR_SYMS 3100   2000   90 1 0
@@@O88   NRST $OSR_SYMS 9600   3400   0 0 0
@@@O89   GND $GND_SYMS 1750   800    90 1 0
@@@O90   GND $GND_SYMS 2700   800    90 0 0
@@@O91   VDD_MCU $PWR_SYMS 3100   1900   90 1 0
@@@O92   VDD_MCU $PWR_SYMS 1400   1900   90 0 0
@@@O93   GND $GND_SYMS 1400   1000   90 1 0
@@@O94   GND $GND_SYMS 3100   1100   90 0 0
@@@O95   GND $GND_SYMS 6000   1800   90 0 0
@@@O96   GND $GND_SYMS 4500   1800   90 1 0
@@@O97   GND $GND_SYMS 5700   2000   90 0 0
@@@O98   GND $GND_SYMS 4800   2000   90 1 0
@@@O99   GND $GND_SYMS 4800   2100   90 1 0
@@@O100  GND $GND_SYMS 5700   2100   90 0 0
@@@O101  VDD_MCU $PWR_SYMS 4750   800    90 0 0
@@@O102  VDD_MCU $PWR_SYMS 4750   900    90 0 0
@@@O103  VDD_MCU $PWR_SYMS 5750   800    90 1 0
@@@O104  VDD_MCU $PWR_SYMS 5750   900    90 1 0
@@@O105  VDD_MCU $PWR_SYMS 6000   1000   90 1 0
@@@O106  VDD_MCU $PWR_SYMS 4400   1000   90 0 0
@@@O107  GND $GND_SYMS 7950   2800   0 0 0
@@@O108  VDD_MCU $PWR_SYMS 10550  5250   0 3 0
@@@O109  PD11 $OSR_SYMS 10550  6900   90 2 0
@@@O110  GND $GND_SYMS 8046   850    0 0 0
@@@O111  PD15_OSC_OUT $OSR_SYMS 7650   1700   0 0 0
@@@O112  PD14_OSC_IN $OSR_SYMS 8500   1700   0 1 0
@@@O113  PD15 $OSR_SYMS 7200   1450   0 0 0
@@@O114  PD14 $OSR_SYMS 8900   1450   0 1 0
@@@O115  PA12 $OSR_SYMS 2800   4300   0 0 0
@@@O116  PD15_OSC_OUT $OSR_SYMS 2800   3900   0 0 0
@@@O117  GND $GND_SYMS 2700   3800   90 1 0
@@@O118  PA14/SWDCK $OSR_SYMS 4800   3600   0 1 0
@@@O119  VDD_MCU $PWR_SYMS 7950   3900   0 0 0
@@@O120  PA0 $OSR_SYMS 7600   3350   0 0 0

*TIEDOTS*



@@@D0    3650   7250  
@@@D1    4500   7250  
@@@D2    4850   7250  
@@@D3    2200   6450  
@@@D4    2400   7250  
@@@D5    3750   6450  
@@@D6    4000   7250  
@@@D7    10100  3400  
@@@D8    3550   7250  
@@@D9    10100  3400  
@@@D10   2400   7250  
@@@D11   2000   7250  
@@@D12   1786   3700  
@@@D13   2136   3138  
@@@D14   2136   3700  
@@@D15   7646   1450  
@@@D16   8046   950   
@@@D17   8446   1450  
@@@D18   7646   1450  
@@@D19   8446   1450  
@@@D20   7950   3350  

*CONNECTION*


*SIGNAL* PA0 0 0
U1.8         @@@O44       2 0
2800   3600  
2800   3600  
J1.12        @@@O78       2 0
2550   1600  
2850   1600  
R30.1        @@@D20       2 0
7950   3350  
7950   3350  
@@@O120      @@@D20       2 0
7600   3350  
7950   3350  
@@@D20       S1.1         2 0
7950   3350  
7950   3450  

*SIGNAL* PA1 0 0
@@@O15       S2.2         2 0
7300   6800  
7300   6600  
U1.9         @@@O43       2 0
3400   3000  
3400   2900  
J1.13        @@@O71       2 0
1950   1500  
1550   1500  

*SIGNAL* MCU_PA10/RX 0 0
U1.31        @@@O36       2 0
3500   4900  
3500   4900  
@@@O64       J2.22        2 0
5750   1100  
5550   1100  

*SIGNAL* MCU_PA9/TX 0 0
U1.30        @@@O42       2 0
3600   4900  
3600   4900  
J2.19        @@@O55       2 0
4950   1200  
4850   1200  

*SIGNAL* PA13/SWDIO 0 0
U1.18        @@@O30       2 0
4700   3700  
4800   3700  
@@@O75       J1.21        2 0
1550   1100  
1950   1100  

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
R8.1         @@@O9        2 0
10100  3950  
10100  3950  
J1.2         @@@O18       2 0
2550   2100  
3100   2100  
J1.1         @@@O19       2 0
1950   2100  
1400   2100  
@@@D12       @@@D14       2 0
1786   3700  
2136   3700  
@@@O4        J3.2         2 0
5450   7250  
5350   7250  
J1.3         @@@O86       2 0
1950   2000  
1400   2000  
J1.4         @@@O87       2 0
2550   2000  
3100   2000  
R14.2        @@@O91       2 0
3050   1900  
3100   1900  
R13.1        @@@O92       2 0
1450   1900  
1400   1900  
J2.27        @@@O101      2 0
4950   800   
4750   800   
J2.25        @@@O102      2 0
4950   900   
4750   900   
J2.28        @@@O103      2 0
5550   800   
5750   800   
J2.26        @@@O104      2 0
5550   900   
5750   900   
R29.2        @@@O105      2 0
6000   1000  
6000   1000  
R28.1        @@@O106      2 0
4500   1000  
4400   1000  
R25.1        @@@O108      2 0
10550  5250  
10550  5250  
C50.2        @@@D12       2 0
1786   3638  
1786   3700  
@@@D12       @@@O39       2 0
1786   3700  
1650   3700  
U1.7         @@@D14       2 0
2800   3700  
2136   3700  
@@@D14       C12.2        2 0
2136   3700  
2136   3638  
S1.2         @@@O119      2 0
7950   3850  
7950   3900  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        @@@D3        2 0
2200   6300  
2200   6450  
@@@O1        R5.2         2 0
4500   6250  
4500   6250  
C31.2        @@@D5        3 0
3650   6550  
3650   6450  
3750   6450  
U2.1         @@@O3        2 0
2750   7050  
2750   6850  
@@@D3        C7.2         3 0
2200   6450  
2000   6450  
2000   6600  
@@@D3        C2.1         3 0
2200   6450  
2400   6450  
2400   6600  
@@@D5        @@@O2        2 0
3750   6450  
3750   6250  
@@@D5        C11.1        3 0
3750   6450  
4000   6450  
4000   6550  
@@@O7        S7.2         3 0
10700  3250  
10700  3400  
10650  3400  
C13.1        @@@O8        2 0
10100  2800  
10100  2800  
R1.2         @@@O11       2 0
9500   5250  
9500   5200  
R6.2         @@@O12       2 0
7300   5700  
7300   5550  
R7.2         @@@O13       2 0
7700   5700  
7700   5550  
R10.2        @@@O14       2 0
8100   5700  
8100   5550  
C12.1        @@@D13       2 0
2136   3138  
2136   3138  
U1.33        @@@O47       2 0
3300   4900  
3300   5030  
J2.5         @@@O57       2 0
4950   1900  
4800   1900  
J2.6         @@@O65       2 0
5550   1900  
5700   1900  
R23.2        @@@O67       2 0
10050  5250  
10050  5200  
J1.25        @@@O76       2 0
1950   900   
1750   900   
J1.24        @@@O84       2 0
2550   1000  
2700   1000  
J1.26        @@@O85       2 0
2550   900   
2700   900   
J1.27        @@@O89       2 0
1950   800   
1750   800   
J1.28        @@@O90       2 0
2550   800   
2700   800   
R16.1        @@@O93       2 0
1500   1000  
1400   1000  
R21.2        @@@O94       2 0
3050   1100  
3100   1100  
R26.2        @@@O95       2 0
6000   1800  
6000   1800  
R27.1        @@@O96       2 0
4500   1800  
4500   1800  
J2.4         @@@O97       2 0
5550   2000  
5700   2000  
J2.3         @@@O98       2 0
4950   2000  
4800   2000  
J2.1         @@@O99       2 0
4950   2100  
4800   2100  
J2.2         @@@O100      2 0
5550   2100  
5700   2100  
R30.2        @@@O107      2 0
7950   2950  
7950   2800  
C50.1        @@@D13       2 0
1786   3138  
2136   3138  
@@@D13       @@@O40       2 0
2136   3138  
2136   3088  
@@@O110      @@@D16       2 0
8046   850   
8046   950   
C10.1        @@@D16       3 0
8446   1050  
8446   950   
8046   950   
@@@D16       C15.1        3 0
8046   950   
7646   950   
7646   1050  
U1.6         @@@O117      2 0
2800   3800  
2700   3800  

*SIGNAL* $$$19650 64 0
R23.1        D2.1         2 0
10050  5650  
10050  5750  

*SIGNAL* $$$19768 64 0
J8.1         D3.1         2 0
10550  6350  
10550  6250  

*SIGNAL* 5V 0 0
J9.1         @@@O5        3 0
1500   7250  
1450   7250  
1450   7300  

*SIGNAL* $$$23084 64 0
R5.1         D4.1         2 0
4500   6650  
4500   6650  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
@@@D0        @@@D6        2 0
3650   7250  
4000   7250  
@@@D0        @@@D8        2 0
3650   7250  
3550   7250  
C31.1        @@@D0        2 0
3650   7050  
3650   7250  
D4.2         @@@D1        2 0
4500   7150  
4500   7250  
@@@D1        @@@D2        2 0
4500   7250  
4850   7250  
@@@D2        J3.3         6 0
4850   7250  
4950   7250  
4950   6950  
5400   6950  
5400   7150  
5350   7150  
@@@O6        @@@D2        3 0
5450   6900  
4850   6900  
4850   7250  
C11.2        @@@D6        2 0
4000   7050  
4000   7250  
@@@D6        @@@D1        2 0
4000   7250  
4500   7250  
U2.2         @@@D8        2 0
3550   7050  
3550   7250  
@@@D8        U2.4         2 0
3550   7250  
3550   7250  

*SIGNAL* NRST 0 0
@@@D9        S7.1         2 0
10100  3400  
10250  3400  
@@@D7        C13.2        2 0
10100  3400  
10100  3300  
R8.2         @@@D7        2 0
10100  3550  
10100  3400  
U1.3         @@@O48       2 0
2800   4100  
2800   4100  
@@@D9        @@@D7        2 0
10100  3400  
10100  3400  
@@@D9        @@@O88       2 0
10100  3400  
9600   3400  

*SIGNAL* $$$2339 64 0
R1.1         D1.1         2 0
9500   5650  
9500   5750  

*SIGNAL* PA2 0 0
@@@O16       S3.2         2 0
7700   6800  
7700   6600  
U1.10        @@@O21       2 0
3500   3000  
3500   2900  
J1.14        @@@O79       2 0
2550   1500  
2850   1500  

*SIGNAL* $$$23311 64 0
R13.2        J1.5         2 0
1850   1900  
1950   1900  

*SIGNAL* $$$13605 64 0
R6.1         S2.1         2 0
7300   6100  
7300   6200  

*SIGNAL* $$$13607 64 0
S3.1         R7.1         2 0
7700   6200  
7700   6100  

*SIGNAL* $$$13609 64 0
S4.1         R10.1        2 0
8100   6200  
8100   6100  

*SIGNAL* $$$978 64 0
R21.1        J1.22        2 0
2650   1100  
2550   1100  

*SIGNAL* $$$979 64 0
J1.23        R16.2        2 0
1950   1000  
1900   1000  

*SIGNAL* $$$23706 64 0
R14.1        J1.6         2 0
2650   1900  
2550   1900  

*SIGNAL* PD15_OSC_OUT 0 0
@@@D15       Y2.2         2 0
7646   1450  
7744   1450  
@@@O111      @@@D15       3 0
7650   1700  
7646   1700  
7646   1450  
C15.2        @@@D18       2 0
7646   1250  
7646   1450  
@@@D18       @@@D15       2 0
7646   1450  
7646   1450  
R9.2         @@@D18       2 0
7550   1450  
7646   1450  
U1.5         @@@O116      2 0
2800   3900  
2800   3900  

*SIGNAL* PD14_OSC_IN 0 0
U1.4         @@@O20       2 0
2800   4000  
2800   4000  
Y2.1         @@@D17       2 0
8344   1450  
8446   1450  
C10.2        @@@D17       2 0
8446   1250  
8446   1450  
@@@D17       @@@D19       2 0
8446   1450  
8446   1450  
@@@D19       @@@O112      3 0
8446   1450  
8446   1700  
8500   1700  
R31.1        @@@D19       2 0
8550   1450  
8446   1450  

*SIGNAL* PA3 0 0
@@@O17       S4.2         2 0
8100   6800  
8100   6600  
U1.12        @@@O23       2 0
3700   3000  
3700   2900  
J1.16        @@@O80       2 0
2550   1400  
2850   1400  

*SIGNAL* PB0 0 0
J6.1         @@@O10       2 0
9500   6750  
9500   6900  
U1.14        @@@O25       2 0
3900   3000  
3900   2900  
J1.18        @@@O81       2 0
2550   1300  
2850   1300  

*SIGNAL* PA12 0 0
J1.8         @@@O77       2 0
2550   1800  
2850   1800  
U1.1         @@@O115      2 0
2800   4300  
2800   4300  

*SIGNAL* $$$17973 64 0
D1.2         J6.2         2 0
9500   6250  
9500   6350  

*SIGNAL* PD15 0 0
@@@O70       J1.11        2 0
1550   1600  
1950   1600  
R9.1         @@@O113      2 0
7250   1450  
7200   1450  

*SIGNAL* PD14 0 0
J1.10        @@@O83       2 0
2550   1700  
2850   1700  
R31.2        @@@O114      2 0
8850   1450  
8900   1450  

*SIGNAL* $$$3495 64 0
U2.3         @@@D4        2 0
2750   7250  
2400   7250  
C7.1         @@@D11       2 0
2000   7100  
2000   7250  
C2.2         @@@D4        2 0
2400   7100  
2400   7250  
@@@D4        @@@D10       2 0
2400   7250  
2400   7250  
@@@D10       J3.1         7 0
2400   7250  
2400   7400  
4950   7400  
4950   7650  
5400   7650  
5400   7350  
5350   7350  
@@@D10       @@@D11       2 0
2400   7250  
2000   7250  
J9.2         @@@D11       2 0
1900   7250  
2000   7250  

*SIGNAL* $$$17989 64 0
D2.2         J7.2         2 0
10050  6250  
10050  6350  

*SIGNAL* $$$1268 64 0
R27.2        J2.7         2 0
4900   1800  
4950   1800  

*SIGNAL* $$$1270 64 0
J2.8         R26.1        2 0
5550   1800  
5600   1800  

*SIGNAL* PB13 0 0
U1.11        @@@O22       2 0
3600   3000  
3600   2900  
@@@O72       J1.15        2 0
1550   1400  
1950   1400  

*SIGNAL* PA11-PC15 0 0
U1.2         @@@O49       2 0
2800   4200  
2800   4200  
J1.9         @@@O68       2 0
1950   1700  
1550   1700  

*SIGNAL* $$$18003 64 0
D3.2         R25.2        2 0
10550  5750  
10550  5650  

*SIGNAL* PA4-PA6 0 0
U1.13        @@@O24       2 0
3800   3000  
3800   2900  
@@@O73       J1.17        2 0
1550   1300  
1950   1300  

*SIGNAL* PB12 0 0
U1.15        @@@O26       2 0
4000   3000  
4000   2900  
@@@O74       J1.19        2 0
1550   1200  
1950   1200  

*SIGNAL* PD0_BOOT0 0 0
U1.16        @@@O45       2 0
4100   3000  
4100   2900  
J1.7         @@@O69       2 0
1950   1800  
1550   1800  

*SIGNAL* $$$1399 64 0
R29.1        J2.24        2 0
5600   1000  
5550   1000  

*SIGNAL* PA14/SWDCK 0 0
J1.20        @@@O82       2 0
2550   1200  
2850   1200  
U1.17        @@@O118      2 0
4700   3600  
4800   3600  

*SIGNAL* $$$1413 64 0
R28.2        J2.23        2 0
4900   1000  
4950   1000  

*SIGNAL* PB4 0 0
U1.19        @@@O29       2 0
4700   3800  
4800   3800  
@@@O58       J2.10        2 0
5750   1700  
5550   1700  
J7.1         @@@O66       2 0
10050  6750  
10050  6900  

*SIGNAL* PB8-PC10 0 0
U1.20        @@@O28       2 0
4700   3900  
4800   3900  
J2.9         @@@O52       2 0
4950   1700  
4850   1700  

*SIGNAL* PC5 0 0
U1.21        @@@O31       2 0
4700   4000  
4800   4000  
@@@O59       J2.12        2 0
5750   1600  
5550   1600  

*SIGNAL* PC6 0 0
U1.22        @@@O27       2 0
4700   4100  
4800   4100  
J2.11        @@@O56       2 0
4950   1600  
4850   1600  

*SIGNAL* PC7 0 0
U1.23        @@@O32       2 0
4700   4200  
4800   4200  
@@@O63       J2.14        2 0
5750   1500  
5550   1500  

*SIGNAL* PD11 0 0
U1.24        @@@O34       2 0
4700   4300  
4800   4300  
J2.13        @@@O51       2 0
4950   1500  
4850   1500  
J8.2         @@@O109      2 0
10550  6750  
10550  6900  

*SIGNAL* PD8 0 0
U1.25        @@@O33       2 0
4100   4900  
4100   4900  
@@@O60       J2.16        2 0
5750   1400  
5550   1400  

*SIGNAL* PD5 0 0
U1.26        @@@O35       2 0
4000   4900  
4000   4900  
J2.15        @@@O53       2 0
4950   1400  
4850   1400  

*SIGNAL* PD4 0 0
U1.27        @@@O38       2 0
3900   4900  
3900   4900  
@@@O61       J2.18        2 0
5750   1300  
5550   1300  

*SIGNAL* PD12 0 0
U1.28        @@@O37       2 0
3800   4900  
3800   4900  
J2.17        @@@O54       2 0
4950   1300  
4850   1300  

*SIGNAL* PD13 0 0
U1.29        @@@O41       2 0
3700   4900  
3700   4900  
@@@O62       J2.20        2 0
5750   1200  
5550   1200  

*SIGNAL* PB3 0 0
U1.32        @@@O46       2 0
3400   4900  
3400   4900  
J2.21        @@@O50       2 0
4950   1100  
4850   1100  

*NETNAMES*



VDD_MCU      @@@O4        400    50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
5V           @@@O5        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_LINK     @@@O6        400    50     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O9        0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O10       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O15       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2          @@@O16       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3          @@@O17       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O18       416    -22    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O19       -400   22     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PD14_OSC_IN  @@@O20       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2          @@@O21       34     -356   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB13         @@@O22       40     -356   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3          @@@O23       40     -358   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA4-PA6      @@@O24       40     -350   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O25       44     -358   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB12         @@@O26       34     -352   90 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC6          @@@O27       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB8-PC10     @@@O28       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB4          @@@O29       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13/SWDIO   @@@O30       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC5          @@@O31       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC7          @@@O32       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD8          @@@O33       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD11         @@@O34       350    50     0 2 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD5          @@@O35       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA10/RX  @@@O36       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD12         @@@O37       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD4          @@@O38       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O39       -408   16     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PD13         @@@O41       0      360    90 8 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA9/TX   @@@O42       0      360    90 8 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O43       -38    -360   90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O44       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD0_BOOT0    @@@O45       -26    -350   90 3 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PB3          @@@O46       0      360    90 8 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
NRST         @@@O48       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA11-PC15    @@@O49       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB3          @@@O50       -364   -6     0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD11         @@@O51       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB8-PC10     @@@O52       -364   34     0 3 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD5          @@@O53       -350   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD12         @@@O54       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA9/TX   @@@O55       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC6          @@@O56       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
GND          J2.5         -500   0      0 1 0      0      0 1 -1 10 97 "Regular Arial Unicode MS"
PB4          @@@O58       350    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC5          @@@O59       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD8          @@@O60       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD4          @@@O61       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD13         @@@O62       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PC7          @@@O63       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
MCU_PA10/RX  @@@O64       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB4          @@@O66       0      360    90 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA11-PC15    @@@O68       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD0_BOOT0    @@@O69       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD15         @@@O70       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA1          @@@O71       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB13         @@@O72       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA4-PA6      @@@O73       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB12         @@@O74       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA13/SWDIO   @@@O75       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O77       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O78       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA2          @@@O79       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA3          @@@O80       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PB0          @@@O81       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/SWDCK   @@@O82       350    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD14         @@@O83       360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O87       420    26     0 7 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O86       -400   -50    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
NRST         @@@O88       -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O91       430    -44    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O92       -402   -38    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O101      -394   30     0 6 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O102      -400   -50    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O103      450    -50    0 5 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O104      450    -50    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O106      -428   -38    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O105      432    -34    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O108      0      -250   0 7 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PD11         @@@O109      0      360    90 8 0      0      90 3 -1 10 97 "Regular Arial Unicode MS"
PD15_OSC_OUT @@@O111      -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD14_OSC_IN  @@@O112      360    0      0 0 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD15         @@@O113      -332   -4     0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD14         @@@O114      360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA12         @@@O115      -360   0      0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PD15_OSC_OUT @@@O116      -360   0      0 9 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
PA14/SWDCK   @@@O118      360    0      0 8 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"
VDD_MCU      @@@O119      0      250    0 4 0      0      0 0 -1 10 97 "Regular Arial Unicode MS"
PA0          @@@O120      -338   -30    0 1 0      0      0 3 -1 10 97 "Regular Arial Unicode MS"

*END*     OF ASCII OUTPUT FILE